Smart Star User's Manual

> A

> - B - C - D - E - F - G - H - I - J - K - L - M - N - O - P - Q - R - S - T - U - V - W - X - Y - Z

> ## Index

> ### A

>   A/D converter card
>     models 1
>   analog input conditioning circuit
>   1
>   anaOutDisable 1

> ### B

>   backplane
>     dimensions 1
>   battery
>     replacing the backup battery
>     1
>   battery backup circuit 1
>   battery connections 1
>   battery life 1

> ### C

>   chip select circuit 1
>   conformal coating 1
>   connections
>     Ethernet cable 1
>     power supply 1
>     programming cable 1
>   CPU card
>     attaching to backplane 1
>     dimensions 1

> ### D

>   D/A converter card
>     analog outputs
>       enabling 1
>     circuit 1
>     models 1
>   digital I/O card 1
>     banks
>       Bank 2 configurations 1
>       locations 1
>     locations of I/O banks 1
>   digital inputs 1
>     pulldown configuration 1
>     pullup configuration 1
>     pullup/pulldown jumper settings 1
>   digital outputs
>     connecting a load 1
>     sinking or sourcing
>       jumper settings 1
>   dimensions
>     A/D converter card 1
>     backplane 1
>     CPU card 1
>     D/A converter card 1
>     digital I/O card 1
>     field wiring terminals 1
>     LCD/keypad module 1, 2
>     LCD/keypad template 1
>     relay cards 1
>   Dynamic C Premier 1, 2, 3, 4, 5, 6, 7
>     basic instructions 1, 2, 3, 4, 5
>     changing programming baud rate in BIOS 1
>     debugging features 1
>     libraries 1, 2, 3, 4, 5
>     starting 1

> ### E

>   Ethernet cables 1
>   Ethernet connections 1
>     10Base-T Ethernet card 1
>     Ethernet hub 1
>     steps 1
>   Ethernet port
>     handling EMI and noise 1
>     pinout 1
>   exclusion zone 1

> ### F

>   features 1
>     A/D converter card 1
>     D/A converter card 1
>     digital I/O card 1
>     relay cards 1
>   field wiring terminals 1, 2
>     guide to FWT selection
>     1, 2
>       A/D converter card 65
>       D/A converter card 83
>       digital I/O card 98
>       relay cards 1
>     installation 1
>     positioning on I/O card 1
>   flash memory
>     liefetime write cycles 1
>   font and bitmap converter 1
>   FWT. See field wiring terminals 1

> ### H

>   headers
>     JP1 1

> ### I

>   I/O address assignments
>     LCD/keypad module 1
>   I/O cards
>     attaching to backplane 1
>   installation
>     CPU card 1
>     field wiring terminals 1
>     I/O cards 1
>   IP addresses 1
>     how to set 1
>     how to set PC IP address 1

> ### J

>   jumper configurations 1
>     JP1 (RS-485 bias and termination resistors) 1, 2
>     JP2 (flash memory bank select) 1
>     JP5 (flash memory bank select) 1
>     jumper locations 1
>   jumper settings
>     digital inputs
>       pullup/pulldown 1
>     digital outputs
>       sinking or sourcing 1

> ### K

>   keypad template 1
>     removing and inserting label
>     1

> ### L

>   LCD/keypad module 1
>     dimensions 1, 2
>     header pinout 1
>     I/O address assignments 1
>     keypad template 1
>     mounting instructions 1
>     removing and inserting keypad label 1
>     sample programs 1

> ### M

>   memory 1
>     flash EPROM configuration for different sizes 1
>     SRAM configuration for different sizes 1
>   models
>     A/D converter card 1
>     D/A converter card 95
>     digital I/O card 1
>     relay cards 1
>   mounting instructions
>     LCD/keypad module 1

> ### O

>   options
>     LCD/keypad module 1

> ### P

>   pinout
>     A/D converter card user interface 1
>     backplane SLOT 0-SLOT 6
>     1
>     CPU card (serial communication) 1
>     D/A converter card user interface 1
>     digital I/O card 1
>       digital outputs 1
>     digital I/O card user interface
>     1
>     Ethernet port 1
>     FWT
>       A/D converter card 1
>       D/A converter card 1
>       digital I/O card 1
>       relay cards 1
>     LCD/keypad module 1
>     programming port 1
>     relay cards 1
>   power distribution
>     A/D converter card 1
>     backplane 1
>     CPU card 1
>     D/A converter card 1
>     digital I/O card 1
>     relay cards 1
>     Smart Star system 1
>   power management 1
>   power supplies
>     backup-battery circuit 1
>     battery backup 1
>     battery backup circuit 1
>     battery life 1
>     chip select circuit 1
>     VRAM switch 1
>   power supply 1
>   Program Mode 1
>   programming
>     flash vs. RAM 1
>     programming cable 1, 2
>     programming port 1
>   programming cable 1, 2, 3
>     DIAG connector 1
>     PROG connector 1
>     switching between Program Mode and Run Mode 1
>   programming port 1
>     pinout 1
>     used as diagnostic port 1

> ### R

>   relay circuit configurations 1
>     diodes 1
>     snubbers 1
>   reset 1
>     reset generator 1
>   RS-232 1
>   RS-485 network 1
>     termination and bias resistors
>     1
>   Run Mode 1

> ### S

>   sample programs 1
>     A/D converter card 1
>       SSTARAD1.C 1
>       SSTARAD2.C 1
>       SSTARAD3.C 1
>     D/A converter card 1
>       ANAVOUT.C 1
>       SSDAC1.C 1
>       SSDAC2.C 1
>       SSDAC3.C 1
>       SSDAC4.C 1
>     digital I/O card 1
>       SSTARIO.C 1
>     how to set IP address 1
>     LCD/keypad module 1
>       ALPHANUN.C 1
>       COFTERMA.C 1
>       DISPPONG.C 1
>       DKADEMO1.C 1
>       FUN.C 1
>       KEYBASIC.C 1
>       KEYMENU.C 1
>       LED.C 1
>       SCROLLING.C 1
>       TEXT.C 1
>     LCD/keypad module (with TCP/IP)
>       MBOXDEMO.C 1, 2
>       TCP_RESPOND.C 1, 2
>       TCPSEND.C 1, 2
>     PONG.C 1
>     relay cards 1
>       SSTARRLY.C 1
>     serial communication
>       MASTER.C 1
>       SLAVE.C 1
>       SSTAR232.C 1
>       SSTAR5W.C 1
>       TCP/IP 1
>         PINGME.C 1
>         SMTP.C 1
>         SSI.C 1
>         SSI2.C 1
>     serial communication
>       programming port 1
>       RS-232 description 1
>       RS-485 description 1
>       RS-485 network 1
>       RS-485 termination and bias resistors 1
>     slot address layout 1
>       A/D converter card 1
>       D/A converter card 1
>       digital I/O card 1
>       relay cards 1
>     software 1, 2, 3, 4, 5
>       A/D converter card 1
>       D/A converter card 1
>       digital I/O card 1, 2
>       digital input APIs 1
>       digital output APIs 1
>       keypad
>         keyConfig 1
>         keyGet 1
>         keyInit 1
>         keypadDef 1
>         keyProcess 1
>         keyScan 1
>         keyUnget 1
>       LCD display
>         glBackLight 1
>         glBlankScreen 1
>         glBlock 1
>         glBuffLock 1
>         glBuffUnlock 1
>         glDispOnOff 1
>         glDown1 1
>         glFillCircle 1
>         glFillPolygon 1
>         glFillScreen 1
>         glFillVPolygon 1
>         glFontCharAddr 1
>         glGetBrushType 1
>         glGetPfStep 1
>         glHScroll 1
>         glInit 1
>         glLeft1 1
>         glPlotCircle 1
>         glPlotDot 1
>         glPlotLine 1
>         glPlotPolygon 1
>         glPlotVPolygon 1
>         glPrintf 1
>         glPutChar 1
>         glPutFont 1
>         glRight1 1
>         glSetBrushType 1
>         glSetContrast 1
>         glSetPfStep 1
>         glSwap 1
>         glUp1 1
>         glVScroll 1
>         glXFontInit 1, 2
>         glXPutBitmap 1, 2
>         glXPutFastmap 1
>         TextCursorLocation 1
>         TextGotoXY 1
>         TextPrintf 1
>         TextPutChar 1
>         TextWindowFrame 1
>       LCD/keypad module
>         ledOut 1
>       LCD/keypad module LEDs 1
>       libraries 1, 2, 3, 4, 5
>         PACKET.LIB 1
>         RS232.LIB 1
>         SMRTSTAR.LIB 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
>       relay cards 1
>       sample programs 1
>         A/D converter card 1
>         D/A converter card 1
>         digital I/O card 1
>         relay cards 1
>       serial communication 1, 2, 3, 4
>       Smart Star bus reset 1
>       Smart Star initialization 1
>       SMRTSTAR.LIB
>         anaIn 1
>         anaInCalib 1
>         anaInEERd 1
>         anaInEEWr 1
>         anaInVolts 1
>         anaLoadCalib 1, 2
>         anaOut 1
>         anaOutCalib 1
>         anaOutDisable 1, 2
>         anaOutEERd 1
>         anaOutEEWr 1
>         anaOutEnable 1, 2
>         anaOutmAmps 1
>         anaOutVolts 1
>         anaSaveCalib 1, 2
>         brdInit 1
>         brdResetBus 1
>         digBankIn 1
>         digBankOut 1
>         digIn 1
>         digOut 1
>         relayOut 1
>         serDRS485Rx 1
>         serDRS485Tx 1
>         serMode 1
>     specifications 1
>       A/D converter card
>         dimensions 1
>         electrical 1
>         temperature 1
>       backplane
>         dimensions 1
>         electrical 1
>         temperature 1
>       CPU card
>         dimensions 1
>         electrical 1
>         mechanical 1
>         temperature 1
>       D/A converter card
>         dimensions 1
>         electrical 1
>         temperature 1
>       digital I/O card
>         dimensions 1
>         electrical 1
>         temperature 1
>       exclusion zone 1
>       field wiring terminals
>         dimensions 1
>       LCD/keypad module
>         dimensions 1, 2
>         electrical 1
>         mechanical 1
>         temperature 1
>         relay cards
>           dimensions 1
>           electrical 1
>           temperature 1
>       subsystems 1

>     ### T

>       TCP/IP connections
>         additional resources 1
>       Tool Kit 1
>         DC power supply 1
>         field wiring terminal 1
>         programming cable 1
>         User's Manual 1

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 757-3792 sales@zworld.com