| RabbitLink User's Manual

> ## Appendix E. Serial Console Commands

> This appendix describes the RabbitLink serial console commands. The serial console was designed to be human-accessible as a convenient way to setup the network configuration. It is possible to use these commands programatically from the target, though it is not recommended. If Internet services are desired, Z-World suggests the DeviceMate software, which may be run on the RabbitLink board.

> ### E.1 Configuration Commands

> These commands are used to set network parameters and to password protect the RabbitLink.

>     set gateway <IP address>
> This command sets the IP address for the gateway.

>     IP address
> | The IP address for the gateway in dotted decimal format. The factory default is `10.10.6.1`.

>     set hostname <name>
> This command allows the RabbitLink to be identified with a unique name, that may be up to 40 characters long.

>     name
> | User-chosen string. The factory default is `RabbitLink`.

>     set ip <IP address>
> This command sets the IP address for the RabbitLink.

>     IP address
> | The IP address for the RabbitLink in dotted decimal format. The factory default is `10.10.1.100`.

>     set netmask x.x.x.x
> This command sets the netmask.

>     x.x.x.x
> | This is the dotted decimal format of the netmask. The factory default is `255.255.255.0`.

>     set passphrase
> This command will prompt for a passphrase twice to confirm that the passphrase was correctly entered. The characters are not echoed back as a security measure. As another security measure, the passphrase is hashed before it is stored on the RabbitLink. Whenever a new session starts with Dynamic C or the RFU, the user will be asked for the passphrase. It should be as long as possible to increase security, up to the maximum length of 255 characters.

>     set port x
> This command sets the TCP port number. If the RabbitLink is being used behind a firewall, it may be necessary to punch a hole in the firewall to allow remote access.

>     x
> | The port number. The factory default is 4244.

>     set dhcp <on | off>
> This command enables and disables the use of any DHCP server that is available on the network. The default condition is `on`. This command is only available with RabbitLink serial console version 2.00.

> ### E.2 Variables Commands

> The RabbitLink serial console has the ability to handle SSI (Server Side Includes) variables. These variables are stored in an xmem buffer. This means that the memory will lose the variables when power is cycled, although the references to the variables will still exist. Remember that any HTML file that includes SSI tags must have the file extension `.shtml`.

>     createv <varname> <vartype> <format> <value> [strlen]
> This command creates a variable and stores it in the flash file system on the RabbitLink. The variable can be referenced in HTML files using SSI; e.g. <!--#echo var="var1"-->).

>     varname
> | The name of the variable.

>     vartype
> | Type of the variable (`int8`, `int16`, `int32`, `float32`, or `string`)

>     format
> | The `printf`-style format specifier (such as `%d`) for outputting the variable

>     value
> | The value to assign to the variable

>     strlen
> | This parameter is used if the variable is of type `string` is used to give the maximum length of the string.
> ### Examples |

>     createv var1 float32 "%.2f" 3.14
>     createv var2 string "%s" "This is a test." 50

>     getv <varname>
> This command gets the value of the specified variable. The value is printed using the format specifier given in the `createv` command.

>     varname
> | The variable whose value is requested.

>     putv <varname> <value>
> This command assigns the specified value to the specified variable.

>     varname
> | The variable whose value is being changed.

>     value
> | The new value for the variable.

>     list variables
> This command lists all the variables by name and type that are stored in the flash file system on the RabbitLink.

>     reset variables
> This command deletes all the variables that are stored in the flash file system on the RabbitLink.

> ### E.3 File Commands

>     delete <filename>
> Deletes the specified file from the flash file system on the RabbitLink.

>     filename
> | Identifies the file to delete.

>     get <filename>
> This command returns the contents of the specified file.

>     filename
> | Identifies the file.

>     list files
> This command lists all the files in the flash file system on the RabbitLink.

>     put <filename>
>     <body of file>
>     <ctrl-D>
> This command sends an ASCII file to the flash file system on the RabbitLink. There is a time-out for this command: the data transfer begins no later than 60 seconds after the RabbitLink senses there is no activity.
> NOTE | It is faster and more efficient to transfer all files, including ASCII files, as binary files.

>     filename
> | Identifies the file.

>     body of file
> | Everything sent before a <`ctrl-D`> (or a <`ctrl-Z`>) is part of the file contents.

>     ctrl-D
>     (or a ctrl-Z)
> | This is the end of file marker.

>     put <filename><size>
> This command sends a binary file to the flash file system on the RabbitLink. There is a time-out for this command: the data transfer begins no later than 60 seconds after the RabbitLink senses there is no activity.
> NOTE | It is faster and more efficient to transfer all files, including ASCII files, as binary files.

>     filename
> | Identifies the file.

>     size
> | The number of bytes in the file being transferred.

> ### E.4 E-Mail Commands

>     mail <e-mail address>
>     <subject>
>     <body>
>     <ctrl-D>
> The mail command sends an e-mail via the RabbitLink to the specified address.

>     e-mail address
> | The address to which the e-mail is sent; e.g. `rabbit@warren.com`.

>     subject
> | After receiving the mail command, the RabbitLink will accept the next string as the subject of the e-mail

>     body
> | After receiving the subject of the e-mail, the RabbitLink will accept strings that follow as the body of the e-mail.

>     ctrl-D
> | `ctrl-D` (0x04) is the end of the e-mail.

>     set mail from <e-mail address>
> This command sets the RabbitLink's e-mail address. The address will be included in the From line of all e-mail messages sent from the RabbitLink. Any error responses from the SMTP server will be sent to this address.

>     e-mail name
> | E-mail address of the RabbitLink; e.g. `rabbit@warren.com`.

>     set mail server <IP address>
> This command sets the IP address of the mail server.

>     IP address
> | The IP address of the mail server in dotted decimal format.

> ### E.5 Other Console Commands

>     echo <on | off>
> This command toggles the echoing of characters.

>     help [filename]
> This command displays the online help.

>     filename
> | This optional parameter limits the help information to that which is associated with the specified file.

>     reset
> This command resets the basic network parameters (the netmask and the IP addresses of the RabbitLink and its gateway) to factory defaults.

>     show [filename]
> This command lists all assignable variables and their settings, except for the passphrase.

>     filename
> | This optional parameter limits the list of variables to those associated with the specified file.

> ### E.6 RabbitLink Console API (prior to Dynamic C 7.20)

> The RabbitLink serial console may be accessed via the serial port using the PROG IN connector on the RabbitLink, as was done in Chapter 2 to configure the RabbitLink.

> If RabbitLink firmware version 1.00 is being used, the API functions described in this section will be recognized by the RabbitLink. Prior to Dynamic C 7.20 these functions were in `STDIO.LIB`.

> ## PrintToConsole

>     int PrintToConsole(char flag);

> This function controls whether STDIO commands such as `printf` go to the RabbitLink serial console in addition to`the Dynamic C` STDIO `window.`

> ### Parameter

> #### flag

> 0-`printf` and related commands work as normal
> `1`-`printf` and related commands go to the RabbitLink serial console as well.

> ### Return Value

> 0 if successful, -1 if not.

> ## SendToConsole

>     int SendToConsole(char *data, int length);

> This function writes a binary buffer of a specified length to the serial console on a RabbitLink. Any data are acceptable since the data will not show up in `the Dynamic C` STDIO `window.`

> ### Parameters

> #### data

> A pointer to the data to be sent.

> #### length

> The length of the buffer passed in data`.`

> ### Return Value

> The actual number of bytes written to the console.

> ## int ConsoleFinish(long timeout);

>     int ConsoleFinish(long timeout);

> This function finishes receiving data from the RabbitLink serial console by blocking for an optional amount of time to do it. If the timeout is set to 0, the function will not receive any data, but will poll to determine whether there are more `data to receive.`

> ### Parameters

> #### timeout

> The length of time to time out, in milliseconds, and is 0 for `ConsoleFinish()` to determine whether there are more data to receive.

> ### Return Value

> 0 if there are more data on the serial console, non-zero if all `the data have been received`.

> ### Library

> STDIO.LIB

> ### E.7 Example Using the RabbitLink Console API

>     main() {
>       // first method
>       SendToConsole("set ip 10.10.2.102\n", 19);

>       // second method
>       PrintToConsole(1);
>       printf("set gateway 10.10.2.1\n");
>       PrintToConsole(0);
>     }

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 757-3792 sales@zworld.com