RabbitCore RCM3000 User's Manual

> A

> - B - C - D - E - F - G - H - I - J - K - L - M - N - O - P - Q - R - S - T - U - V - W - X - Y - Z

> ## Index

> ### A

>   additional information
>     Getting Started manual 1
>     online documentation 1
>   auxiliary I/O bus 1

> ### B

>   battery backup
>     battery life 1
>     external battery connections 1
>     reset generator 1
>   bus loading 1

> ### C

>   clock doubler 1
>   conformal coating 1

> ### D

>   Development Kit
>     RCM2200 1
>   digital I/O 1
>     I/O buffer sourcing and sinking limits 1
>     memory interface 1
>     SMODE0 1, 2
>     SMODE1 1, 2
>   dimensions
>     LCD/keypad module 1
>     LCD/keypad template 1
>     Prototyping Board 1
>     RCM3000 1
>   Dynamic C 1
>     libraries 1
>     upgrades and patches 1

> ### E

>   Ethernet port 1
>     pinout 1
>   exclusion zone 1

> ### F

>   features 1
>   flash memory addresses
>     use blocks 1

> ### I

>   I/O address assignments
>     LCD/keypad module 1
>   I/O buffer sourcing and sinking limits 1

> ### J

>   jumper configurations 1
>     JP1 (flash memory bank select) 1, 2
>     JP2 (flash memory size) 1
>     JP3 (flash memory size) 1
>     JP4 (SRAM size) 1
>     JP5 (auxiliary I/O data bus) 1
>     jumper locations 1

> ### K

>   keypad template 1
>     removing and inserting label 1

> ### L

>   LCD/keypad module
>     dimensions 1
>     header pinout 1
>     I/O address assignments 1
>     keypad template 1
>     mounting instructions 1
>     removing and inserting keypad label 1
>     sample programs 1

> ### M

>   manuals 1
>   motor control option
>     quadrature decoder 1
>   mounting instructions
>     LCD/keypad module 1

> ### P

>   physical mounting 1
>   pin 1 locations 1
>   pinout
>     Ethernet port 1
>     LCD/keypad module 1
>     programming cable 1
>     Prototyping Board 1
>     RCM3000
>       alternate configurations 1, 2
>     RCM3000 headers 1
>   power supplies
>     +3.3 V 1
>     battery backup 1
>     optional +5 V output 1
>   Program Mode 1
>     switching modes 1
>   programming cable 1, 2
>     DIAG connector 1
>     pinout 1
>   programming port 1
>     alternate pinout configurations 1
>     used as diagnostic port 1
>   Prototyping Board
>     adding RS-232 transceiver 1
>     attach modules 1
>     dimensions 1
>     J6
>       pinout 1
>     motor control option 1
>     pinout 1
>     power supply 1
>     prototyping area 1
>     specifications 1
>   PWM outputs 1
>   PWM registers 1

> ### Q

>   quadrature decoder 1
>   quadrature decoder registers 1

> ### R

>   Rabbit 3000
>     data and clock delays 1
>     Parallel Port F Registers 1
>     Parallel Port F registers 1
>     PWM outputs 1
>     PWM registers 1
>     quadrature decoder registers 1
>     spectrum spreader time delays 1
>   Rabbit subsystems 1
>   Run Mode 1
>     switching modes 1

> ### S

>   sample programs
>     LCD/keypad module 1
>   serial communication 1
>   serial ports 1
>     Ethernet port 1
>     programming port 1
>   software
>     auxiliary I/O bus 1, 2, 3
>     I/O drivers 1
>     keypad
>       keyConfig 1
>       keyGet 1
>       keyInit 1
>       keypadDef 1
>       keyProcess 1
>       keyScan 1
>       keyUnget 1
>     LCD display
>       glBackLight 1
>       glBlankScreen 1
>       glBlock 1
>   software
>     LCD display (continued)
>       glBuffLock 1
>       glBuffUnlock 1
>       glDispOnOff 1
>       glDown1 1
>       glFillCircle 1
>       glFillPolygon 1
>       glFillScreen 1
>       glFillVPolygon 1
>       glFontCharAddr 1
>       glGetBrushType 1
>       glGetPfStep 1
>       glHScroll 1
>       glInit 1
>       glLeft1 1
>       glPlotCircle 1
>       glPlotDot 1
>       glPlotLine 1
>       glPlotPolygon 1
>       glPlotVPolygon 1
>       glPrintf 1
>       glPutChar 1
>       glPutFont 1
>       glRight1 1
>       glSetBrushType 1
>       glSetContrast 1
>       glSetPfStep 1
>       glSwap 1
>       glUp1 1
>       glVScroll 1
>       glXFontInit 1
>       glXPutBitmap 1
>       glXPutFastmap 1
>       TextCursorLocation 1
>       TextGotoXY 1
>       TextPrintf 1
>       TextPutChar 1
>       TextWindowFrame 1
>     LCD/keypad module
>       ledOut 1
>     LCD/keypad module LEDs
>     1
>   software (continued)
>     libraries 1
>       PACKET.LIB 1
>       RCM3000.LIB 1
>       RS232.LIB 1
>       TCP/IP 1
>     readUserBlock 1
>     sample programs 1
>       PONG.C 1
>       RCM3000 1
>       TCPIP 1
>     serial communication drivers 1
>     TCP/IP drivers 1
>     writeUserBlock 1
>   specifications 1
>     bus loading 1
>     digital I/O buffer sourcing and sinking limits 1
>     dimensions 1
>     electrical, mechanical, and environmental 1
>     exclusion zone 1
>     header footprint 1
>     headers 1
>     LCD/keypad module
>       dimensions 1
>       electrical 1
>       mechanical 1
>       temperature 1
>     physical mounting 1
>     pin 1 locations 1
>     Prototyping Board 1
>     Rabbit 3000 DC characteristics 1
>     Rabbit 3000 timing diagram 1
>     relative pin 1 locations 1
>   spectrum spreader 1
>   subsystems
>     digital inputs and outputs 1
>   switching modes 1

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 757-3792 sales@zworld.com | Rabbit Semiconductor http://www.rabbitsemiconductor.com Voice: (530) 757-8400 FAX: (530) 757-8402 sales@rabbitsemiconductor.com