Wildcat (BL2000) User's Manual

> ## Appendix D. Demonstration Board

> Appendix D shows how to connect the Demonstration Board to the BL2000.

> ### D.1 Connecting Demonstration Board

> Before running sample programs based on the Demonstration Board, you will have to connect the Demonstration Board from the BL2000 Tool Kit to the BL2000 board. Proceed as follows.

> 1. Use the wires included in the BL2000 Tool Kit to connect header J1 on the Demonstration Board to header J8 and J9 on the BL2000. The connections are shown in Figure D-1 for sample programs DIGIN.C, DIGOUT.C, and SMTP.C, and in Figure D-2 for sample program ANADIGIN.C.
> 2. Make sure that your BL2000 is connected to your PC and that the power supply is connected to the BL2000 and plugged in as described in Chapter 2, "Getting Started."

> Figure D-1. General Digital Connections Between BL2000 and Demonstration Board

> Figure D-2. Analog Connections Between BL2000 and Demonstration Board

Z-World http://www.zworld.com Voice: (530) 753-3737 FAX: (530) 753-5141 sales@zworld.com