Intellicom User's Manual

> A

> - B - C - D - E - F - G - H - I - J - K - L - M - N - O - P - Q - R - S - T - U - V - W - X - Y - Z

> ## Index

> ### A

>   AC adapter 1, 2

> ### B

>   backup battery board 1
>     replacing 1
>   battery backup circuit 1
>   battery connections 1
>   battery life 1
>   bezel 1
>     disammbling Intellicom 1

> ### C

>   chip select circuit 1
>   conduit 1
>   conformal coating 1
>   connections
>     Ethernet cable 1
>     power supply 1, 2
>     programming cable 1

> ### D

>   Demonstration Board 1
>     hookup instructions 1
>   demonstration program 1
>   digital inputs 1
>     pullup/pulldown configuration 1
>   digital outputs 1
>     sinking 1
>   dimensions
>     bezel 1
>     front panel 1
>     Intellicom board 1
>     outer casing 1
>   display
>     vacuum fluorescent display option 1, 2
>   Dynamic C Premier 1, 2
>     basic instructions 1
>     break point 1
>     changing programming baud rate in BIOS 1
>     debugging features 1
>     editing the program 1
>     features 1
>     handling different memories in BIOS 1
>     libraries 1
>       ARP.LIB 1
>       ICOM.LIB 1, 2
>       TCPIP.LIB 1
>     memory
>       BIOS 1
>     multitasking 1, 2
>     programming in flash vs. RAM 1
>     single-stepping 1
>     starting 1
>     watch expression 1
>     watching variables dynamically 1

> ### E

>   Ethernet cables 1, 2
>   Ethernet connections 1, 2
>     Ethernet cable 1
>     steps 1

> ### F

>   features 1
>   front panel bezel dimensions 1

> ### H

>   headers
>     JP1 1

> ### I

>   I/O pinout 1
>   Intellicom
>     features
>       software demonstration 1
>     introduction 1
>   introduction 1
>   IP addresses 1, 2
>     how to set 1
>     how to set PC IP address 1

> ### J

>   jumper configurations 1, 2
>     JP1 (RS-485 bias and termination resistors) 1
>     JP1 (SRAM size) 1
>     JP2 (flash memory bank select) 1
>     JP2 (flash memory size) 1
>     JP3 (flash memory size) 1
>     JP4 (digital input pull-up/pull-down resistors) 1
>     JP5 (flash memory bank select) 1
>     JP6 (RS-485 bias and termination resistors) 1
>     JP7 (RS-232/RS-485 select) 1
>     jumper locations 1

> ### K

>   keypad
>     disassembling from bezel 1
>   keypad insert 1
>     changing 1
>   keypad matrix 1

> ### M

>   memory 1
>     BIOS 1
>     flash EPROM configuration for different sizes 1
>     SRAM configuration for different sizes 1
>   models 1
>     OP6600 1
>     OP6700 1

> ### O

>   OP6600 1
>   OP6700 1
>   outer casing
>     removal 1

> ### P

>   pin configurations
>     programming port 1
>   pinout
>     Ethernet port 1
>     I/O 1
>     programming port 1
>     RJ-12 connector 1
>     RJ-45 connector 1
>     serial communication 1
>   plastic casing 1, 2, 3
>     assembly 1, 2
>     attaching conduit 1
>     Ethernet cable 1
>     mounting 1
>     mounting brackets 1
>     watertight mounting 1
>   power management 1
>   power supplies 1
>     Backup battery board 1
>     battery backup 1
>     battery backup circuit 1
>     battery life 1
>     chip select circuit 1
>     switching voltage regulator 1
>     VRAM switch 1
>   power-up
>     demonstration program 1
>   Program Mode 1
>   programming
>     flash vs. RAM 1
>     programming cable 1, 2
>     programming port 1
>   programming cable
>     DIAG connector 1
>   programming port
>     pin configurations 1
>     pinout 1
>     used as diagnostic port 1

> ### R

>   reset 1, 2, 3
>     reset generator 1
>   RS-232 1
>   RS-485 1
>     termination and bias resistors 1
>   RS-485 network 1
>   Run Mode 1
>   running TCP/IP sample programs 1

> ### S

>   sample programs 1
>     COFTERMA.C 1
>     DEMOBRD1.C 1, 2, 3
>     DEMOBRD2.C 1, 2
>     DEMOBRD3.C 1, 2
>     how to run 1
>     how to set IP address 1
>     HTTPDEMO.C 1
>     ICOM232.C 1
>     ICOM485.C 1
>     ICOM5WIRE.C 1
>     ICOMDEMO.C 1, 2
>     ICOMIO.C 1
>     KEYLCD.C 1
>     MBOXDEMO.C 1
>     MUSIC.C 1
>     MUSIC2.C 1
>     PINGME.C 1
>     PONG.C 1
>     power-up demonstration program 1
>     REMOTE1.C 1
>     running TCP/IP sample programs 1
>     RXSAMPLE.C 1
>     SAMPLES\ICOM\WINDOWS directory 1
>     SMTPDEMO.C 1
>     SPEAKER.C 1
>     SSI3.C 1
>     STATIC.C 1
>     TCP/IP 1
>     TCP_RESPOND.C 1, 2
>     TCP_SEND.C 1, 2
>     using PCRESPOND 1
>     using PCSEND 1
>   serial communication 1
>     programming port 1
>     RS-232 description 1
>     RS-232/RS-485 options 1, 2, 3
>     RS-485 description 1
>     RS-485 network 1, 2
>       common power supply 1
>     RS-485 termination and bias resistors 1
>   serial communication pinout 1
>   software 1
>     board initialization 1
>       brdInit 1
>     digital I/O 1
>       digIn 1
>       digOut 1
>     display controls 1
>       dispClear 1
>       dispContrast 1
>       dispCursor 1
>       dispGoto 1
>       dispOnoff 1
>       dispPrintf 1
>       dispPutc 1
>     keypad controls 1
>       keyConfig 1
>       keyGet 1
>       keyInit 1
>       keypadDef 1
>       keyProcess 1
>     libraries
>       ARP.LIB 1
>       BOOTP.LIB 1
>       BSDNAME.LIB 1
>       DCRTCP.LIB 1
>       DNS.LIB 1
>       FTP_CLIENT.LIB 1
>       FTP_SERVER.LIB 1
>       HTTP.LIB 1
>       ICMP.LIB 1
>       IP.LIB 1
>       MD5.LIB 1
>       NET.LIB 1
>       PACKET.LIB 1
>       PKTDRV.LIB 1
>       POP3.LIB 1
>       REALTEK.LIB 1
>       RS232.LIB 1
>       SMTP.LIB 1
>       TCP.LIB 1
>       UDP.LIB 1
>       VSERIAL.LIB 1
>       ZSERVER.LIB 1
>   software (continyed)
>     serial communication 1
>       serB485Rx 1
>       serB485Tx 1
>       serMode 1
>     speaker controls 1
>       spkrOut 1
>   speaker 1
>     output characteristics 1
>   specifications 1
>     electrical 1
>     front panel bezel dimensions 1
>     mechanical dimensions Intellicom board 1
>     outer casing dimensions 1
>     temperature 1
>   subsystems 1

> ### T

>   TCP/IP connections 1, 2, 3
>     10BaseT 1
>     10BaseT Ethernet card 1
>     additional resources 1
>     Ethernet cable 1
>     Ethernet cables 1
>     Ethernet hub 1
>     IP addresses 1, 2
>     steps 1
>   template
>     keypad insert 1
>   Tool Kit 1
>     AC adapter 1
>     Demonstration Board 1
>     programming cable 1
>     User's Manual 1
>     wire assembly 1

> ### V

>   vacuum fluorescent display 1, 2
>     changing PCB configuration 1

> ### W

>   watertight mounting 1

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 757-3792 sales@zworld.com