Here is a list of all documented class members with links to the class documentation for each member:

### - a -

- Addr : Digi.Drivers.I2CiMX51

### - b -

- Block : Digi.Drivers.GPIO , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51

### - c -

- ClockRate : Digi.Drivers.I2CiMX51
- Close() : Digi.Common.DriverIO
- CreateFile() : Digi.Common.DriverIO
- CTL_CODE() : Digi.Imported.WINIOCTL_H

### - d -

- DeviceIOControl() : Digi.Common.DriverIO
- Direction : Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIO
- DirectionValue : Digi.Drivers.GPIO
- DisableSlave() : Digi.Drivers.I2CiMX51
- DriveStrength : Digi.Drivers.GPIOiMX51
- DriveStrengthValue : Digi.Drivers.GPIOiMX51

### - e -

- EnableSlave() : Digi.Drivers.I2CiMX51

### - f -

- FileHandle : Digi.Common.DriverIO
- Frequency : Digi.Drivers.I2CiMX51

### - g -

- GetSlaveText() : Digi.Drivers.I2CiMX51
- GPIO() : Digi.Drivers.GPIO
- GPIO_IOEXPANSORiMX51() : GPIO_IOEXPANSORiMX51
- GPIOiMX51() : Digi.Drivers.GPIOiMX51

### - h -

- Hysteresis : Digi.Drivers.GPIOiMX51

### - i -

- I2C() : Digi.Drivers.I2C
- I2CiMX51() : Digi.Drivers.I2CiMX51
- I2CPort : Digi.Drivers.I2CiMX51
- I2CResult : Digi.Drivers.I2CiMX51
- InMode : Digi.Drivers.GPIOiMX51
- Invert : GPIO_IOEXPANSORiMX51
- IoValue : Digi.Drivers.GPIO
- IrqMode : Digi.Drivers.GPIO , Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51
- IrqModeIXM51 : Digi.Drivers.GPIOiMX51
- IrqValue : Digi.Drivers.GPIOiMX51 , Digi.Drivers.GPIO
- IsMaster() : Digi.Drivers.I2CiMX51
- IsSlave() : Digi.Drivers.I2CiMX51

### - l -

- Length : Digi.Drivers.I2CiMX51

### - o -

- OpenDrain : Digi.Drivers.GPIOiMX51
- OutVoltage : Digi.Drivers.GPIOiMX51

### - p -

- Poll() : Digi.Drivers.GPIO , Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51
- Port : Digi.Drivers.GPIOiMX51
- PullUpDown : Digi.Drivers.GPIOiMX51
- PullUpDownValue : Digi.Drivers.GPIOiMX51

### - r -

- Read() : Digi.Drivers.I2C , Digi.Drivers.I2CiMX51
- ReadFile() : Digi.Common.DriverIO
- Refresh() : Digi.Drivers.WatchDog
- Release() : Digi.Drivers.GPIOiMX51
- Reset() : Digi.Drivers.I2CiMX51
- Result : Digi.Drivers.I2CiMX51
- RW : Digi.Drivers.I2CiMX51
- RWOperation : Digi.Drivers.I2CiMX51

### - s -

- SelfAddress : Digi.Drivers.I2CiMX51
- SetMasterMode() : Digi.Drivers.I2CiMX51
- SetSlaveMode() : Digi.Drivers.I2CiMX51
- SetSlaveText() : Digi.Drivers.I2CiMX51
- SlaveSize : Digi.Drivers.I2CiMX51
- SlewRate : Digi.Drivers.GPIOiMX51
- Start() : Digi.Drivers.WatchDog

### - v -

- Value : Digi.Drivers.GPIO , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51

### - w -

- Wait() : Digi.Drivers.GPIO , Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51
- WakeUpValue : Digi.Drivers.GPIOiMX51
- WatchDog() : Digi.Drivers.WatchDog
- WatchDogAction : Digi.Drivers.WatchDog
- Write() : Digi.Drivers.I2C , Digi.Drivers.I2CiMX51
- WriteFile() : Digi.Common.DriverIO