### - c -

- Close() : Digi.Common.DriverIO
- CreateFile() : Digi.Common.DriverIO
- CTL_CODE() : Digi.Imported.WINIOCTL_H

### - d -

- DeviceIOControl() : Digi.Common.DriverIO
- DisableSlave() : Digi.Drivers.I2CiMX51

### - e -

- EnableSlave() : Digi.Drivers.I2CiMX51

### - g -

- GetSlaveText() : Digi.Drivers.I2CiMX51
- GPIO() : Digi.Drivers.GPIO
- GPIO_IOEXPANSORiMX51() : GPIO_IOEXPANSORiMX51
- GPIOiMX51() : Digi.Drivers.GPIOiMX51

### - i -

- I2C() : Digi.Drivers.I2C
- I2CiMX51() : Digi.Drivers.I2CiMX51
- IsMaster() : Digi.Drivers.I2CiMX51
- IsSlave() : Digi.Drivers.I2CiMX51

### - p -

- Poll() : Digi.Drivers.GPIO , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51

### - r -

- Read() : Digi.Drivers.I2C , Digi.Drivers.I2CiMX51
- ReadFile() : Digi.Common.DriverIO
- Refresh() : Digi.Drivers.WatchDog
- Release() : Digi.Drivers.GPIOiMX51
- Reset() : Digi.Drivers.I2CiMX51

### - s -

- SetMasterMode() : Digi.Drivers.I2CiMX51
- SetSlaveMode() : Digi.Drivers.I2CiMX51
- SetSlaveText() : Digi.Drivers.I2CiMX51
- Start() : Digi.Drivers.WatchDog

### - w -

- Wait() : Digi.Drivers.GPIO , Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51
- WatchDog() : Digi.Drivers.WatchDog
- Write() : Digi.Drivers.I2C , Digi.Drivers.I2CiMX51
- WriteFile() : Digi.Common.DriverIO