- Addr : Digi.Drivers.I2CiMX51
- Block : Digi.Drivers.GPIO , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51
- ClockRate : Digi.Drivers.I2CiMX51
- Direction : Digi.Drivers.GPIO , Digi.Drivers.GPIOiMX51 , GPIO_IOEXPANSORiMX51
- DriveStrength : Digi.Drivers.GPIOiMX51
- Frequency : Digi.Drivers.I2CiMX51
- Hysteresis : Digi.Drivers.GPIOiMX51
- InMode : Digi.Drivers.GPIOiMX51
- Invert : GPIO_IOEXPANSORiMX51
- IrqMode : GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51 , Digi.Drivers.GPIO
- IrqModeIXM51 : Digi.Drivers.GPIOiMX51
- Length : Digi.Drivers.I2CiMX51
- OpenDrain : Digi.Drivers.GPIOiMX51
- OutVoltage : Digi.Drivers.GPIOiMX51
- PullUpDown : Digi.Drivers.GPIOiMX51
- Result : Digi.Drivers.I2CiMX51
- RW : Digi.Drivers.I2CiMX51
- SelfAddress : Digi.Drivers.I2CiMX51
- SlaveSize : Digi.Drivers.I2CiMX51
- SlewRate : Digi.Drivers.GPIOiMX51
- Value : Digi.Drivers.GPIO , GPIO_IOEXPANSORiMX51 , Digi.Drivers.GPIOiMX51