Show Contents

# 2.3. Set up DEY debugger

Follow these steps to configure the Digi Embedded Yocto debugger:

1. Click Tools > Options.
2. Select Build & Run from the list at the left.
3. In the right pane, select the Debuggers tab.
4. Click Add in the right pane to add a new debugger.
5. Enter a name to identify the new debugger, for example <PLATFORM>_DEY_GDB.
6. Click Browse to fill the debugger path. A file system explorer dialog opens.

7. Navigate through your file system and select the arm-dey-linux-gnueabi-gdb binary installed within your platform toolchain, usually located at:

       <toolchain_installation_path>/sysroots/x86_64-deysdk-linux/usr/bin/arm-dey-linux-gnueabi/arm-dey-linux-gnueabi-gdb

8. Click Apply to save the new debugger.

© 2018 Digi International Inc. All rights reserved.
2.3. Set up DEY debugger updated on 14 February 2018 12:04:14 AM