Show Contents

# Digi Embedded Yocto for the ConnectCore 6UL SBC Pro

Digi Embedded Yocto is an embedded Linux distribution that uses the community open source Yocto Project. The Digi Embedded Yocto distribution includes the following components:

- A Linux kernel for Digi's embedded hardware products
- The U-Boot bootloader for Digi's embedded hardware products
- Reference root file system images
- A C/C++ cross-compilation toolchain

This section contains all the documentation you need to flash Yocto in your device and work with it.

Digi Embedded Yocto in a nutshell
Learn more about the Yocto Project and how Digi supports your product development.
Get started
Program Yocto into your ConnectCore 6UL device and boot it for the first time.
System development
Install Yocto and take the first steps with the ConnectCore 6UL device to create and build your own Yocto image.
Application development
Discover the various ways to develop applications using the Yocto Project along with helpful guidelines.
TrustFence™ for Digi Embedded Yocto
Integrate device security, device identity, and data privacy capabilities on your ConnectCore 6UL.
Remote management
Remotely monitor and manage your devices with integrated Remote Manager support.
FAQ
Get answers to the most common and frequently asked questions related to the ConnectCore 6UL platform and Yocto.