Show Contents

# Set up your development workstation

You must first set up your PC workstation to use Digi Embedded Yocto. The resulting environment enables cross-platform development for ConnectCore devices using a Linux workstation.

- 1. Connect the hardware
- 2. Install required packages
- 3. Set up a TFTP server
- 4. Set up a NFS server

## Requirements

- A 64-bit Linux machine with Internet connection.
- A Linux distribution supported by the Yocto Project.

Digi Embedded Yocto is developed using Ubuntu 16.04 LTS.

For successful Digi Embedded Yocto projects, Digi recommends you use a Yocto Project-supported Ubuntu distribution. You can find Yocto Project-supported distributions in the Yocto Project system requirements at http://www.yoctoproject.org/docs/2.2/ref-manual/ref-manual.html#detailed-supported-distros.

- 8 GB of RAM.
- 8 CPU cores.
- 250 GB of free disk space. SSDs are highly recommended for faster build times.

## 1. Connect the hardware

Connect the cable.

This system boots the Linux kernel, device trees, and other boot artifacts from a TFTP server and mounts a root filesystem from a NFS server. This is ideal for development; changes to either the Linux kernel image or the root filesystem are immediately available without having to program the target device.

## 2. Install required packages

Install the following list of required packages for Ubuntu 16.04 Linux distribution:

    ~> sudo apt-get install gawk wget git-core diffstat unzip texinfo gcc-multilib build-essential chrpath socat libsdl1.2-dev xterm minicom

Note If you are using a different Linux distribution, find the list of packages at http://www.yoctoproject.org/docs/2.2/ref-manual/ref-manual.html#required-packages-for-the-host-development-system.

## 3. Set up a TFTP server

You also need to set up a TFTP server on your host so you can program your built images.

1. Install a TFTP server.
   For Ubuntu 16.04, you can execute the following command to install a TFTP server:

    ~> sudo apt-get install tftpd-hpa

2. After completing installation, create a directory /tftpboot where exported files will be located (only root user can create this directory):

    ~> sudo mkdir /tftpboot
    ~> sudo chmod 1777 /tftpboot

3. To make sure the TFTP server is using the /tftpboot directory, edit the daemon's configuration file /etc/default/tftpd-hpa and change the constant TFTP_DIRECTORY to point to your recently created /tftpboot folder:

    /etc/default/tftpd-hpa

    TFTP_USERNAME="tftp"
    TFTP_DIRECTORY="/tftpboot"
    TFTP_ADDRESS="0.0.0.0:69"
    TFTP_OPTIONS="--secure"

4. Restart the daemon so that it uses the new TFTP folder:

    ~> sudo service tftpd-hpa restart
    tftpd-hpa start/running, process 3297

## 4. Set up a NFS server

Booting from NFS during system development can significantly reduce idle time compared to flashing an image directly in your device.

Follow these steps in your Linux machine to install and configure the NFS server:

1. Install the NFS server:

    ~> sudo apt-get install nfs-kernel-server

2. Create a directory to use as root of the NFS server, for example, /export/nfsroot.

    ~> sudo mkdir -p /export/nfsroot

3. Export the whole /exports/nfsroot directory. To do so, edit the /etc/exports file of your development machine as root and add the following line:

    /export/nfsroot/ *(rw,no_root_squash,async,no_subtree_check)

4. Restart the NFS server with the following command:

    ~> sudo service nfs-kernel-server restart

© 2018 Digi International Inc. All rights reserved.
Set up your development workstation updated on 22 January 2018 05:11:29 PM