Show Contents

# Wi-Fi configuration

Note This section contains Linux BSP documentation for kernel v4.1. Click here for v4.9 BSP documentation.

You can use the NetworkManager tool to configure the wireless device. The NetworkManager package also includes a command line tool, nmcli, which you can use to interact with the NetworkManager daemon.

By default, Digi Embedded Yocto is configured with concurrent station, soft AP, and P2P capabilities. When using concurrent mode, the interface is shared between all functionalities so overall performance is affected.

CAUTION! Maximum performance is achieved on the physical wlan0 when the wireless interface is not shared between multiple functionalities. Digi recommends you always use the physical wlan0 interface and only configure virtual interfaces when using concurrent modes.

© 2018 Digi International Inc. All rights reserved.
Wi-Fi configuration updated on 22 January 2018 02:43:37 PM