Show Contents

# Known issues and limitations

Note This section contains Linux BSP documentation for kernel v4.1. Click here for v4.9 BSP documentation.

- In kernel v4.9, peer-to-peer Autonomous Group Owner (Autonomous GO) configuration fails due to an incompatibility in the wireless driver. Digi recommends you use the Negotiated Group Owner (Negotiated GO) method.

- The QCA6564 wireless chip does not support Wake on Wireless LAN.
- When using concurrent mode, performance is reduced because the wireless interface is shared between several different functionalities.
- When using concurrent mode, Digi recommends you keep the different modes on the same frequency channels. For example, when configuring access point mode on channel 36 on band A, Digi recommends you connect to the same channel both in station mode and WiFi direct to optimize radio performance.
- When working as an access point, DFS-capable channels in band A are not currently supported.

© 2018 Digi International Inc. All rights reserved.
Known issues and limitations updated on 22 January 2018 02:43:37 PM