Show Contents

# U-Boot bootloader

The ConnectCore 6UL platform uses U-Boot (Universal Bootloader) as its primary bootloader. U-Boot is an open-source project. You can find standard documentation about commands, environment variables, Flattened Device Tree support, and more at www.denx.de/wiki/U-Boot/Documentation.

## About this guide

This guide only describes specific changes made to the standard U-Boot by Digi International.

## Version

U-Boot for ConnectCore 6UL is based on standard U-Boot v2015.04 plus NXP patches at git.freescale.com/git/cgit.cgi/imx/uboot-imx.git.

## Supported interfaces

The U-Boot for ConnectCore 6UL supports the following interfaces:

- UART5 for console (115200/8/N/1)
- DDR3
- NAND Flash
- uSD card (on USDHC2)
- 10/100Mbps Ethernet on SMSC LAN8720 PHY (RGMII)
- I2C multi-port
- One-Time-Programmable (OTP) bits

## Carrier board version and ID

Digi uses several OTP bits to code the carrier board version and ID. See Carrier board version and ID.

© 2018 Digi International Inc. All rights reserved.
U-Boot bootloader updated on 22 January 2018 04:10:26 PM