Show Contents

# Network configuration

Note This section contains Linux BSP documentation for kernel v4.1. Click here for v4.9 BSP documentation.

## MAC addresses

Digi programs one MAC address during manufacturing of the SOM. This is the MAC address used for the wlan0 interface. The wireless chip supports up to three other virtual MAC addresses that you must program before use (otherwise they have default values). See Wireless virtual MAC addresses for instructions.

## IP settings

Digi Embedded Yocto defines configuration macros to set some of the most commonly used network interface settings. See Customize the root file system. By default, wlan0 is configured to obtain a DHCP address.

You can also configure additional network interface settings by editing /etc/NetworkManager/system-connections/<Config_File. You can also use the nmcli tool, which is part of the NetworkManager package.

© 2018 Digi International Inc. All rights reserved.
Network configuration updated on 22 January 2018 02:43:37 PM