Show Contents

# 2.2. Set up DEY compilers

- 1. Configure DEY Qt Compiler
- 2. Configure DEY C Compiler
- 3. Configure DEY C++ Compiler

## 1. Configure DEY Qt Compiler

Follow these steps to configure the Digi Embedded Yocto Qt compiler:

1. Click Tools > Options.
2. Select Build & Run from the list at the left.
3. In the right pane, select the Qt Versions tab
4. Click Add to add a new Qt compiler.
5. Navigate through your file system and select the qmake binary installed within your platform toolchain, usually located at:

       <toolchain_installation_path>/sysroots/x86_64-deysdk-linux/usr/bin/qt5/qmake

6. Click Apply to save the new Qt compiler.

Note If you receive a warning message stating that there was already a configured binary for the same Qt version, ignore it and close the popup.

## 2. Configure DEY C Compiler

Follow these steps to configure the Digi Embedded Yocto C compiler:

1. Click Tools > Options.
2. Select Build & Run from the list at the left.
3. In the right pane, select the Compilers tab
4. Click Add and select GCC > C from the drop-down menu to add a new C native compiler.
5. Enter a name to identify the new C compiler, for example <PLATFORM>_DEY_GCC.
6. Click Browse to fill the C compiler path. A file system explorer dialog opens.
7. Navigate through your file system and select the arm-dey-linux-gnueabi-gcc binary installed within your platform toolchain, usually located at:

       <toolchain_installation_path>/sysroots/x86_64-deysdk-linux/usr/bin/arm-dey-linux-gnueabi/arm-dey-linux-gnueabi-gcc

8. Click Apply to save the new C compiler.

## 3. Configure DEY C++ Compiler

Follow these steps to configure the Digi Embedded Yocto C++ compiler:

1. Click Tools > Options.
2. Select Build & Run from the list at the left.
3. In the right pane, select the Compilers tab
4. Click Add and select GCC > C++ from the drop-down menu to add a new C++ native compiler.
5. Enter a name to identify the new C++ compiler, for example <PLATFORM>_DEY_G++.
6. Click Browse to fill the C++ compiler path. A file system explorer dialog opens.
7. Navigate through your file system and select the arm-dey-linux-gnueabi-g++ binary installed within your platform toolchain, usually located at:

       <toolchain_installation_path>/sysroots/x86_64-deysdk-linux/usr/bin/arm-dey-linux-gnueabi/arm-dey-linux-gnueabi-g++

8. Click Apply to save the new C++ compiler.

© 2018 Digi International Inc. All rights reserved.
2.2. Set up DEY compilers updated on 22 January 2018 02:43:38 PM