
============================================
| Test Harness Main Options:               |
|   c - (C)ontinuous transmit mode         |
|   r - Continuous RF (R)eceive mode       |
|   l - (L)ink test menu                   |
|   t - (T)hroughput test menu             |
|   h - C(h)ain Menu                       |
|   e - Load (E)EPROM Calibration          |
|   s - (S)witch test card                 |
|   m - (M)anufacturing/Calibration Test   |
|   p - EE(P)ROM function                  |
|   g - Disable lo(g)ging                  |
|   w - (W)rite Comment to Log File        |
|   u - (U)tility Menu                     |
|   i - (N)oise Immunity Menu              |
|   b - (B)luetooth Test                   |
|   q - (Q)uit                             |
============================================
SNOOP: rateindex=0, datarate=0x6

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 125 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 121 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 121 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 120 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x1d: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 119 
SNOOP: rateindex=48, datarate=0x80

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 
SNOOP: rateindex=49, datarate=0x81

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 27 MCS 1 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 27 MCS 1 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 27 MCS 1 HT40 1S, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 27 MCS 1 HT40 1S, PN9 thermVal 121 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 27 MCS 1 HT40 1S, PN9 thermVal 120 
SNOOP: rateindex=50, datarate=0x82

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 40.5 MCS 2 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 40.5 MCS 2 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 40.5 MCS 2 HT40 1S, PN9 thermVal 121 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 40.5 MCS 2 HT40 1S, PN9 thermVal 120 
SNOOP: rateindex=51, datarate=0x83

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 54 MCS 3 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 54 MCS 3 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 54 MCS 3 HT40 1S, PN9 thermVal 123 
SNOOP: rateindex=52, datarate=0x84

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 81 MCS 4 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 81 MCS 4 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 81 MCS 4 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 81 MCS 4 HT40 1S, PN9 thermVal 122 
SNOOP: rateindex=53, datarate=0x85

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 108 MCS 5 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 108 MCS 5 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 108 MCS 5 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 108 MCS 5 HT40 1S, PN9 thermVal 122 
SNOOP: rateindex=54, datarate=0x86

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 121.5 MCS 6 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 121.5 MCS 6 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 121.5 MCS 6 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 121.5 MCS 6 HT40 1S, PN9 thermVal 123 
SNOOP: rateindex=55, datarate=0x87

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9 thermVal 124 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 135 MCS 7 HT40 1S, PN9 thermVal 122 
SNOOP: rateindex=48, datarate=0x80

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 123 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 121 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 120 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   % - Toggle Control/Ext/Dup      | - Toggle Short GI         |
|   ^ - Swap Control & Extension    ~ - Toggle C&E separation   |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx), HT40, |E-20-C|, CTL

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0xa: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 
SNOOP: rateindex=48, datarate=0x80

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 120 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate = 13.5 MCS 0 HT40 1S, PN9 thermVal 117 
SNOOP: rateindex=0, datarate=0x6

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9
=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 122 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 120 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 119 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 118 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 117 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 116 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 116 

=================================================================
| Continuous Transmit Options                                   |
|   p - Increase Center Frequency by 5 MHz                      |
|   l - Decrease Center Frequency by 5 MHz                      |
|   4 - Toggle HT40 Mode                                        |
|   | - Toggle Short GI                                         |
|   o - Increase Data Rate (O - next rate mode)                 |
|   k - Decrease Data Rate (K - last rate mode)                 |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   s - Toggle output mode (frame | tx99 | single carrier)      |
|   a - Toggle antenna                                          |
|   $ - Toggle forcedPAL                                        |
|   # - Toggle PAPRD                                            |
|   ^ - dump regs                                               |
|   d - Toggle Data Pattern                                     |
|   z - Toggle Scramble mode                                    |
|   : - Cycle up dac IQ constant values (511 - 2047) (; - down) |
|   ! - Enter STBC mode                                         |
| ESC - exit                                                    |
=================================================================

Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)

Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x9: 
ANT_A, [TX99], Rate =  6 Mbps, PN9 thermVal 116 

Exit Continuous Mode .....

============================================
| Test Harness Main Options:               |
|   c - (C)ontinuous transmit mode         |
|   r - Continuous RF (R)eceive mode       |
|   l - (L)ink test menu                   |
|   t - (T)hroughput test menu             |
|   h - C(h)ain Menu                       |
|   e - Load (E)EPROM Calibration          |
|   s - (S)witch test card                 |
|   m - (M)anufacturing/Calibration Test   |
|   p - EE(P)ROM function                  |
|   g - Disable lo(g)ging                  |
|   w - (W)rite Comment to Log File        |
|   u - (U)tility Menu                     |
|   i - (N)oise Immunity Menu              |
|   b - (B)luetooth Test                   |
|   q - (Q)uit                             |
============================================
exiting
