
============================================
| Test Harness Main Options:               |
|   c - (C)ontinuous transmit mode         |
|   r - Continuous RF (R)eceive mode       |
|   l - (L)ink test menu                   |
|   t - (T)hroughput test menu             |
|   h - C(h)ain Menu                       |
|   e - Load (E)EPROM Calibration          |
|   s - (S)witch test card                 |
|   m - (M)anufacturing/Calibration Test   |
|   p - EE(P)ROM function                  |
|   g - Disable lo(g)ging                  |
|   w - (W)rite Comment to Log File        |
|   u - (U)tility Menu                     |
|   i - (N)oise Immunity Menu              |
|   b - (B)luetooth Test                   |
|   q - (Q)uit                             |
============================================

=================================================================
| Link Test Mode                                                |
|   t - Tx                                                      |
|   r - Rx                                                      |
|   R - Rx for Signal generator                                 |
|   0 - Rx for Promiscous mode                                  |
|   p - Increase Center Frequency by 5 MHz (P inc by 100 MHz)   |
|   l - Decrease Center Frequency by 5 MHz (L dec by 100 MHz)   |
|   4 - Toggle HT40 Mode                                        |
|   5 - Toggle Shared Rx Mode                                   |
|   6 - Toggle BT CO-EX Mode                                    |
|   3 - Toggle for EVM display                                  |
|   i - Increase pcdac (I inc by 10)                            |
|   j - Decrease pcdac (J dec by 10)                            |
|   f - Increase power output by 0.5dBm (F inc by 5dBm)         |
|   c - Decrease power output by 0.5dBm (C dec by 5dBm)         |
|   u - Increase ob by 1 (w - increase b-ob)                    |
|   h - Increase db by 1 (q - increase b-db)                    |
|   o - Next Rates (k - Last Rates)  RateMask: All Rates        |
|   z - Toggle packet interleave                                |
|   a - Toggle antenna                                          |
|   + - Cycle screen width:  80 chars                           |
| ESC - exit                                                    |
=================================================================
Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)


Operating in 11g at channel 2.412GHz, Chain masks: 0x1(Tx), 0x1(Rx)
Power control mode:
PCDAC = 30, ext power detector = 0,
ob5g=1 d2b5g=1 d3b5g=1 d4b5g=1 
ob2g_paloff=3 ob2g_qam=2 ob2g_psk=3 ob2g_cck=6 db2g=5
forcedPAL=Off sharedRx=Off btCoEx=Off paprd2G=Disabled paprd5G=Disabled (0x0: 
Selected rate mask All Rates    
Freq = 2412, ANT_A, pkt interleave: on
Begin receiving packets for infinite loops, displayed as good packets(RSSI)

         Signal Generator Receive Mode (Unicast&Broadcast)

     2 - Enable RX log
     7 - change, now MAC_ADDRESS: 0X     8 - change, now BSSID: 0X     E - Reset the pkt count		  
     p - Increase Center Frequency by 5 MHz (P inc by 100 MHz)   
     l - Decrease Center Frequency by 5 MHz (L dec by 100 MHz)   
     Esc - Press Esc to return 		  

Receiving in 11g at channel 2.412GHz
Total receive packet number:		0
Good Packet number:			0
Bad packet number:			0
Crc error packet number:		0
Decrypt error packet number:		0
Phy error packet number:		0

Error: rxGetStats 0: no stats


         Signal Generator Receive Mode (Unicast&Broadcast)

     2 - Enable RX log
     7 - change, now MAC_ADDRESS: 0X     8 - change, now BSSID: 0X     E - Reset the pkt count		  
     p - Increase Center Frequency by 5 MHz (P inc by 100 MHz)   
     l - Decrease Center Frequency by 5 MHz (L dec by 100 MHz)   
     Esc - Press Esc to return 		  

Receiving in 11g at channel 2.412GHz
Total receive packet number:		0
Good Packet number:			0
Bad packet number:			0
Crc error packet number:		0
Decrypt error packet number:		0
Phy error packet number:		0

Error: rxGetStats 0: no stats


         Signal Generator Receive Mode (Unicast&Broadcast)

     2 - Enable RX log
     7 - change, now MAC_ADDRESS: 0X     8 - change, now BSSID: 0X     E - Reset the pkt count		  
     p - Increase Center Frequency by 5 MHz (P inc by 100 MHz)   
     l - Decrease Center Frequency by 5 MHz (L dec by 100 MHz)   
     Esc - Press Esc to return 		  

Receiving in 11g at channel 2.412GHz
Total receive packet number:		0
Good Packet number:			0
Bad packet number:			0
Crc error packet number:		0
Decrypt error packet number:		0
Phy error packet number:		0

Error: rxGetStats 0: no stats


         Signal Generator Receive Mode (Unicast&Broadcast)

     2 - Enable RX log
     7 - change, now MAC_ADDRESS: 0X     8 - change, now BSSID: 0X     E - Reset the pkt count		  
     p - Increase Center Frequency by 5 MHz (P inc by 100 MHz)   
     l - Decrease Center Frequency by 5 MHz (L dec by 100 MHz)   
     Esc - Press Esc to return 		  

Receiving in 11g at channel 2.412GHz
Total receive packet number:		0
Good Packet number:			0
Bad packet number:			0
Crc error packet number:		0
Decrypt error packet number:		0
Phy error packet number:		0

Error: rxGetStats 0: no stats

exiting

============================================
| Test Harness Main Options:               |
|   c - (C)ontinuous transmit mode         |
|   r - Continuous RF (R)eceive mode       |
|   l - (L)ink test menu                   |
|   t - (T)hroughput test menu             |
|   h - C(h)ain Menu                       |
|   e - Load (E)EPROM Calibration          |
|   s - (S)witch test card                 |
|   m - (M)anufacturing/Calibration Test   |
|   p - EE(P)ROM function                  |
|   g - Disable lo(g)ging                  |
|   w - (W)rite Comment to Log File        |
|   u - (U)tility Menu                     |
|   i - (N)oise Immunity Menu              |
|   b - (B)luetooth Test                   |
|   q - (Q)uit                             |
============================================
exiting
