# target power file for AR6003nx_2 802.11n Reference Design card



# 11a Target Power table : 

#	 Rules:

#		1. up to a maximum of 8 test frequencies

#		2. test frequencies DO NOT need to cover the entire range of 5180-5850. It

#		   is allowed to provide data for a smaller range. for all channels

#		   outside of test frequencies range, target power will be assumed 0dB.

#		3. specify mask/PER limited target power for various rates

#

#BEGIN_11a_TARGET_POWER_TABLE  

#  test_frequencies   6-24_target  36_target 48_target   54_target  

								     

   5180         	14        14       14          13

   5320			14        14       14          13

   5700			14        14       14          13

   5825			14        14       14          13



#END_11a_TARGET_POWER_TABLE



# 11b Target Power table : 

#	 Rules:

#		1. Need to define exactly 2 test frequencies in 2.412 - 2.484 G range. 

#		2. test frequencies DO NOT need to cover the entire range of 2412-2484. It

#		   is allowed to provide data for a smaller range. for all channels

#		   outside of test frequencies range, target power will be assumed 0dB.

#		3. specify mask/PER limited target power for various rates

#

#BEGIN_11b_TARGET_POWER_TABLE  

#  test_frequencies   1L_target  2M_target 5.5M_target   11M_target  

							       

   2412			14	    14	     14	       14      

   2484			14	    14	     14	       14      



#END_11b_TARGET_POWER_TABLE



# ofdm@2p4 Target Power table : 

#	 Rules:

#		1. up to a maximum of 3 test frequencies in 2.412 - 2.484 G range

#		2. test frequencies DO NOT need to cover the entire range of 2412-2484. It

#		   is allowed to provide data for a smaller range. for all channels

#		   outside of test frequencies range, target power will be assumed 0dB.

#		3. specify mask/PER limited target power for various rates

#

#BEGIN_11g_TARGET_POWER_TABLE  

#  test_frequencies   6-24_target  36_target 48_target   54_target  

								    

   2412			14	    14     	13	13  

   2437			14	    14     	13	13

   2472			14	    14     	13	13	    



#END_11g_TARGET_POWER_TABLE



# HT 2GHz and 5GHz Target Power table : 

#	 Rules:

#		1. up to a maximum of 4 test frequencies in 2.412 - 2.484 G and 4900 - 5900 G range

#		2. test frequencies DO NOT need to cover the entire range of frequency. It

#		   is allowed to provide data for a smaller range. for all channels

#		   outside of test frequencies range, target power will be assumed 0dB.

#		3. specify mask/PER limited target power for various rates

#BEGIN_5GHZ_HT20_TARGET_POWER_TABLE  

#  test_frequencies     MCS 0/8  MCS 1/9  MCS 2/10  MCS 3/11  MCS 4/12  MCS 5/13  MCS 6/14  MCS 7/15     

								    

   5180			  13       13       13        13          13        13       13      12

   5240			  13       13       13        13          13        13       13      12

   5320			  13       13       13        13          13        13       13      12

   5500			  13       13       13        13          13        13       13      12

   5700			  13       13       13        13          13        13       13      12

   5745			  13       13       13        13          13        13       13      12

   5825			  13       13       13        13          13        13       13      12



#END_5GHZ_HT20_TARGET_POWER_TABLE  





#BEGIN_5GHZ_HT40_TARGET_POWER_TABLE  

#  test_frequencies     MCS 0/8  MCS 1/9  MCS 2/10  MCS 3/11  MCS 4/12  MCS 5/13  MCS 6/14  MCS 7/15     



   5190			  13       13       13        13          13        13       13      12

   5230			  13       13       13        13          13        13       13      12

   5270			  13       13       13        13          13        13       13      12

   5510			  13       13       13        13          13        13       13      12

   5670			  13       13       13        13          13        13       13      12

   5755			  13       13       13        13          13        13       13      12

   5795			  13       13       13        13          13        13       13      12



#END_5GHZ_HT40_TARGET_POWER_TABLE  



#BEGIN_2GHZ_HT20_TARGET_POWER_TABLE  

#  test_frequencies     MCS 0/8  MCS 1/9  MCS 2/10  MCS 3/11  MCS 4/12  MCS 5/13  MCS 6/14  MCS 7/15     

								    

       2412             14       14       14        14          12        12        10       10

       2437             14       14       14        14          12        12        10       10

       2472             14       14       14        14          12        12        10       10

       



#END_2GHZ_HT20_TARGET_POWER_TABLE



#BEGIN_2GHZ_HT40_TARGET_POWER_TABLE  

#  test_frequencies     MCS 0/8  MCS 1/9  MCS 2/10  MCS 3/11  MCS 4/12  MCS 5/13  MCS 6/14  MCS 7/15     

								    

       2412             14       14       14        14          12        12        10       10

       2437             14       14       14        14          12        12        10       10

       2472             14       14       14        14          12        12        10       10



#END_2GHZ_HT40_TARGET_POWER_TABLE









# Test Groups :

#      Rules:

#		1. Specify up to 8 band edges for each test group.

#		2. If no backoff desired at a band edge, give a large number (e.g, 30) so

#		   that the driver determined limit becomes the target power.

#



#BEGIN_TEST_GROUPS





# Test Group 1: US and CANADA (FCC) 802.11a mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6     BE7	BE8        

	0x10	    	5180	5200	5320	5500	5600	5700    5745	5825

                        8.5     15      15      15      15      15      16.5 	16.5	# Band Edge Max Power

     		    	0	1    	0	1    	1	1       1  	0	# in-band flag



# Test Group 2: US and CANADA (FCC) 802.11n HT20 5GHz mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6     BE7	BE8        

	0x16	    	5180	5200	5320	5500	5600	5700    5745	5825

                        10      16      17      17      17      17      16 	16	# Band Edge Max Power

     		    	0	1    	0	1    	1	1       1  	0	# in-band flag



# Test Group 3: US and CANADA (FCC) 802.11n HT40 5GHz mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6     BE7	BE8        

	0x18	    	5190	5230	5310	5510	5590	5670    5755	5795

                        12.5    16.5    17      17      17      17      16 	16	# Band Edge Max Power

     		    	0	1    	0	1    	1	0       1  	1	# in-band flag



# Test Group 4: US and CANADA (FCC) 802.11b mode CTL

# test_group_code	BE1   	BE2	BE3	

	0x11	    	2412    2417    2462		

        		17	19	17.5	# Band Edge Max Power

			0	1	0	# in-band flag



# Test Group 5: US and CANADA (FCC) 802.11g mode CTL

# test_group_code	BE1	BE2	BE3		

	0x12		2412	2417	2462		

			15	18	14		# Band Edge Max Power

			0	1	0		# in-band flag



# Test Group 6: US and CANADA (FCC) 802.11n HT20 2GHz mode CTL

# test_group_code   	BE1	BE2	BE3	

        0x15           	2412    2417    2462		

                    	15      18      12.5     	# Band Edge Max Power

                    	0       1       0	 	# in-band flag



# Test Group 7: US and CANADA (FCC) 802.11n HT40 2GHz mode CTL

# test_group_code   	BE1	BE2	BE3     BE4     

        0x17           	2422    2427    2447    2452

                    	12      18      18      10.5  	# Band Edge Max Power

                    	0       1       1       0   	# in-band flag#END_TEST_GROUPS



# Test Group 8: Japan (MKK) 802.11a mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	        

	0x40	    	5170	5200	5260	5320	

                        13      13      13      13      # Band Edge Max Power

     		    	1	1    	1	1    	# in-band flag



# Test Group 9: Japan (MKK) 802.11n HT20 5GHz mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	     

	0x46	    	5170	5200	5260	5320	

                        13.5    13.5    13.5    13.5    # Band Edge Max Power

     		    	1	1    	1	1    	# in-band flag



# Test Group 10: Japan (MKK) 802.11b mode CTL

# test_group_code	BE1   	BE2	BE3	BE4	

	0x41	    	2412    2417    2472	2484		

        		15	15	15	15	# Band Edge Max Power

			0	1	0	0	# in-band flag



# Test Group 11: Japan (MKK) 802.11g mode CTL

# test_group_code	BE1	BE2	BE3		

	0x42		2412	2417	2472		

			16.5	16.5	16.5		# Band Edge Max Power

			0	1	0		# in-band flag



# Test Group 12: Japan (MKK) 802.11n HT20 2GHz mode CTL

# test_group_code   	BE1	BE2	BE3	

        0x45           	2412    2417    2452		

                    	17      17      17      	# Band Edge Max Power

                    	0       1       0	 	# in-band flag



# Test Group 13: Europe (ETSI) 802.11a mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6     BE6	BE7     

	0x30	    	5180	5260	5320	5500	5600	5700    5745	5825

                        14.5    14.5    14.5    16.5    16.5    16.5    16.5	16.5 		# Band Edge Max Power

     		    	0	1    	0	1    	1	1       1	0		# in-band flag



# Test Group 14: Europe (ETSI) 802.11n HT20 5GHz mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6      BE6	BE7       

	0x36	    	5180	5200	5320	5500	5600	5700     5745	5825

                        14.5    14.5    14.5    16.5    16.5    16.5     16.5	16.5		# Band Edge Max Power

     		    	0	1    	0	1    	1	1        1      0		# in-band flag



# Test Group 15: Europe (ETSI) 802.11n HT40 5GHz mode CTL

#	test_group_code	BE1	BE2	BE3	BE4	BE5	BE6     

	0x38	    	5190	5230	5310	5510	5590	5670    

                        14.5    14.5    14.5    16.5    16.5    16.5      		# Band Edge Max Power

     		    	0	1    	0	1    	1	0       		# in-band flag



# Test Group 16: Europe (ETSI) 802.11b mode CTL

# test_group_code	BE1   	BE2	BE3	

	0x31	    	2412    2417    2472		

        		14	14	14	# Band Edge Max Power

			0	1	0	# in-band flag



# Test Group 17: Europe (ETSI) 802.11g mode CTL

# test_group_code	BE1	BE2	BE3		

	0x32		2412	2417	2472		

			14	14	14		# Band Edge Max Power

			0	1	0		# in-band flag



# Test Group 18: Europe (ETSI) 802.11n HT20 2GHz mode CTL

# test_group_code   	BE1	BE2	BE3	

        0x35           	2412    2417    2472		

                    	14      14      14       	# Band Edge Max Power

                    	0       1       0	 	# in-band flag



# Test Group 19: Europe (ETSI) 802.11n HT40 2GHz mode CTL

# test_group_code   	BE1	BE2	BE3     BE4     

        0x37           	2422    2427    2447    2452

                    	14      14      14      14   	# Band Edge Max Power

                    	0       1       1       0   	# in-band flag#END_TEST_GROUPS



#END_TEST_GROUPS



