Following Issues have been fixed since version 3.2.12.0e:
- Wireless driver does NOT receive broadcast packets when the AP is configured with mixed TKIP AES encryption.

Following Issues have been fixed since version 3.2.12.0d:
- Fix to make CCWMX53 module work: 
  Force write operations to use single block because of host controller multiblock issues.


Following Issues have been fixed since version 3.2.12.0c:
- Limit eu_regdom to 13 dBm for 2.4GHz and 10 dBm for 5GHz.


Following Issues have been fixed since version 3.2.12.0b:
- Updated wireless rsfilter.
- Removed internal debugging code in ganges_pause() function.
- ticket#02996: Version 3.2.12.0 breaks what was solved on ticket #02243: 
  Long time to reconnect to an AP after de-authentication.


Following Issues have been fixed since version 3.2.12.0a:
- Jira WCE-52: MX51 does not enter in suspend:
  queue_netbuffer_for_send(): Skip sending non EAP packets when using WPA 
  while keys are not yet installed.

Changes introduced by Digi from Redpine release 3.2.12.0 to create 3.2.12.0a:
- Digi customizations: MAC address loading, interface name...
- MAX_NUM_OF_NODES increased from 100 to 300
- Added Registry to increase beacon_miss_count from 20 to 400
