Update process for 3.2.12.1b release:
-------------------------------------
- Dll update:
  In the 'dll' folder from this zip, choose '\QFE_December2014_Wave2\CCWMXWIFI.dll' file
  and copy it to '_TARGETPLATROOT\Files' folder in your PC.

  Note that this dll requires QFEs installed up to December2014 (Also known as Wave2) or later.

- Firmware update:
  Replace _PLATFORMROOT\common\src\soc\COMMON_DIGI\DRIVERS\Redpine folder in your PC with the '\firmware\Redpine' folder from this zip.
- Sysgen the project to make sure the project use latest installed QFEs.
- Check on new boot that the wireless driver reports 3.2.12.1a version

