ID: 138
Name: BSP_Updates_752
Version: 1.00
Dependences: none
Description: Version 1.0@@@Removed calls to the IOP queue flush routines.  The latest version of the IOP driver does these calls itself when the naIopProcessorStopAndReset is called.  Calling the flush routines a second time can cause buffers to be duplicated, and that can cause the CAN driver to panic.  This has been seen on tests when the CAN bus was opened and closed repeatedly. (Case 40284)@@@Corrected a problem with RF chip type checking.@@@Updated TODO messages for checking authorities in fileinit.c, and adding a semaphore to protect access on the download image if needed in firmware.c. Removed TODO for file type in firmware.c. (Case 39705)         @@@Corrected issue that caused naCliAddUserTable() to improperly overwrite commands when using -O2 optimization. (Case 38136)@@@Fixed lockup condition in Ethernet bypass transmit, and changed code for the example application to make it more readable. (Case 37952)@@@
Minidescription: BSP Updates since the release of NET+OS 7.5.2
platformversion: 7.5
Revision: 2
platform: netos
Relevance: NORMAL
Filename: BSP_Updates_752_138.dipk
Date: 02/12/2011
Type: fix
Target: environment
Size: 179kb
Installedsize: 817kb
Checksum: aad7275ba8db9b87b96f9c2acb9662d4
