No.     Time        Source                Destination           Protocol Info
      6 1.031928    10.10.10.50           10.10.10.58           SNMP     trap

Frame 6 (135 bytes on wire, 135 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:13.506303000
    [Time delta from previous captured frame: 0.000758000 seconds]
    [Time delta from previous displayed frame: 0.000758000 seconds]
    [Time since reference or first frame: 1.031928000 seconds]
    Frame Number: 6
    Frame Length: 135 bytes
    Capture Length: 135 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:snmp]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 121
    Identification: 0x000c (12)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x51e9 [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 60153 (60153), Dst Port: snmptrap (162)
    Source port: 60153 (60153)
    Destination port: snmptrap (162)
    Length: 101
    Checksum: 0xa5cd [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Simple Network Management Protocol
    version: version-1 (0)
    community: public
    data: trap (4)

No.     Time        Source                Destination           Protocol Info
      7 1.034663    10.10.10.50           10.10.10.58           SNMP     sNMPv2-Trap

Frame 7 (117 bytes on wire, 117 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:13.509038000
    [Time delta from previous captured frame: 0.002735000 seconds]
    [Time delta from previous displayed frame: 0.002735000 seconds]
    [Time since reference or first frame: 1.034663000 seconds]
    Frame Number: 7
    Frame Length: 117 bytes
    Capture Length: 117 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:snmp]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 103
    Identification: 0x000d (13)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x51fa [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 54771 (54771), Dst Port: snmptrap (162)
    Source port: 54771 (54771)
    Destination port: snmptrap (162)
    Length: 83
    Checksum: 0xc116 [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Simple Network Management Protocol
    version: v2c (1)
    community: public
    data: sNMPv2-Trap (7)

No.     Time        Source                Destination           Protocol Info
      8 1.037761    10.10.10.50           10.10.10.58           SNMP     sNMPv2-Trap

Frame 8 (210 bytes on wire, 210 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:13.512136000
    [Time delta from previous captured frame: 0.003098000 seconds]
    [Time delta from previous displayed frame: 0.003098000 seconds]
    [Time since reference or first frame: 1.037761000 seconds]
    Frame Number: 8
    Frame Length: 210 bytes
    Capture Length: 210 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:snmp]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 196
    Identification: 0x000e (14)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x519c [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 44006 (44006), Dst Port: snmptrap (162)
    Source port: 44006 (44006)
    Destination port: snmptrap (162)
    Length: 176
    Checksum: 0xe015 [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Simple Network Management Protocol
    msgVersion: snmpv3 (3)
    msgGlobalData
    msgAuthoritativeEngineID: 80001770010A342079000000000000000000000000
    msgAuthoritativeEngineBoots: 7
    msgAuthoritativeEngineTime: 3893
    msgUserName: Trap User
    msgAuthenticationParameters: <MISSING>
    msgPrivacyParameters: <MISSING>
    msgData: plaintext (0)




No.     Time        Source                Destination           Protocol Info
     22 9.693424    10.10.10.50           10.10.10.58           SNMP     trap

Frame 22 (295 bytes on wire, 295 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:22.167799000
    [Time delta from previous captured frame: 0.113551000 seconds]
    [Time delta from previous displayed frame: 0.113551000 seconds]
    [Time since reference or first frame: 9.693424000 seconds]
    Frame Number: 22
    Frame Length: 295 bytes
    Capture Length: 295 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:snmp]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 281
    Identification: 0x000f (15)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x5146 [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 34996 (34996), Dst Port: snmptrap (162)
    Source port: 34996 (34996)
    Destination port: snmptrap (162)
    Length: 261
    Checksum: 0xe84b [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Simple Network Management Protocol
    version: version-1 (0)
    community: public
    data: trap (4)

No.     Time        Source                Destination           Protocol Info
     23 9.698433    10.10.10.50           10.10.10.58           SNMP     sNMPv2-Trap

Frame 23 (277 bytes on wire, 277 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:22.172808000
    [Time delta from previous captured frame: 0.005009000 seconds]
    [Time delta from previous displayed frame: 0.005009000 seconds]
    [Time since reference or first frame: 9.698433000 seconds]
    Frame Number: 23
    Frame Length: 277 bytes
    Capture Length: 277 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:snmp]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 263
    Identification: 0x0010 (16)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x5157 [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 37225 (37225), Dst Port: snmptrap (162)
    Source port: 37225 (37225)
    Destination port: snmptrap (162)
    Length: 243
    Checksum: 0x55d4 [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Simple Network Management Protocol
    version: v2c (1)
    community: public
    data: sNMPv2-Trap (7)

No.     Time        Source                Destination           Protocol Info
     24 9.701783    10.10.10.50           10.10.10.58           UDP      Source port: 50597  Destination port: snmptrap

Frame 24 (368 bytes on wire, 368 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:22.176158000
    [Time delta from previous captured frame: 0.003350000 seconds]
    [Time delta from previous displayed frame: 0.003350000 seconds]
    [Time since reference or first frame: 9.701783000 seconds]
    Frame Number: 24
    Frame Length: 368 bytes
    Capture Length: 368 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:data]
    [Coloring Rule Name: UDP]
    [Coloring Rule String: udp]
Ethernet II, Src: Digiboar_2e:6d:d4 (00:40:9d:2e:6d:d4), Dst: Dell_84:dc:61 (00:1c:23:84:dc:61)
Internet Protocol, Src: 10.10.10.50 (10.10.10.50), Dst: 10.10.10.58 (10.10.10.58)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 354
    Identification: 0x0011 (17)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 64
    Protocol: UDP (0x11)
    Header checksum: 0x50fb [correct]
    Source: 10.10.10.50 (10.10.10.50)
    Destination: 10.10.10.58 (10.10.10.58)
User Datagram Protocol, Src Port: 50597 (50597), Dst Port: snmptrap (162)
    Source port: 50597 (50597)
    Destination port: snmptrap (162)
    Length: 334
    Checksum: 0x42c2 [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
Data (326 bytes)

0000  30 82 00 42 02 01 03 30 82 00 0d 02 01 00 02 02   0..B...0........
0010  07 d0 04 01 00 02 01 03 04 31 30 82 00 2d 04 15   .........10..-..
0020  80 00 17 70 01 0a 34 20 79 00 00 00 00 00 00 00   ...p..4 y.......
0030  00 00 00 00 00 02 01 07 02 02 0f 3d 04 09 54 72   ...........=..Tr
0040  61 70 20 55 73 65 72 04 00 04 00 30 82 00 f7 04   ap User....0....
0050  15 80 00 17 70 01 0a 34 20 79 00 00 00 00 00 00   ....p..4 y......
0060  00 00 00 00 00 00 04 00 a7 82 00 da 02 01 00 02   ................
0070  01 00 02 01 00 30 82 00 cd 30 82 00 0f 06 08 2b   .....0...0.....+
0080  06 01 02 01 01 03 00 43 03 05 f4 32 30 82 00 18   .......C...20...
0090  06 0a 2b 06 01 06 03 01 01 04 01 00 06 0a 2b 06   ..+...........+.
00a0  01 04 01 ae 70 01 03 01 30 82 00 10 06 0a 2b 06   ....p...0.....+.
00b0  01 04 01 ae 70 01 03 01 02 02 10 10 30 82 00 1e   ....p.......0...
00c0  06 0b 2b 06 01 04 01 ae 70 01 03 02 01 04 0f 56   ..+.....p......V
00d0  61 6c 75 65 20 6f 66 20 4f 49 44 20 23 33 30 82   alue of OID #30.
00e0  00 64 06 0b 2b 06 01 04 01 ae 70 01 03 02 02 06   .d..+.....p.....
00f0  55 2b 06 01 04 01 ae 70 01 03 03 00 00 81 85 a3   U+.....p........
0100  24 81 82 f9 18 02 81 a6 d5 10 c0 85 fa 30 81 82   $............0..
0110  f9 38 81 82 f8 7c c0 a6 e6 24 c0 91 c9 18 02 00   .8...|...$......
0120  02 81 a6 d5 10 01 02 02 02 02 81 a6 d5 10 01 02   ................
0130  81 82 f9 54 81 82 f9 3c c0 a6 99 78 c0 a6 e2 44   ...T...<...x...D
0140  02 02 81 82 fa 10                                 ......
    Data: 308200420201033082000D020100020207D0040100020103...

No.     Time        Source                Destination           Protocol Info
     25 10.329861   10.10.10.58           10.255.255.255        NBNS     Registration NB W_ACU_CARGED<20>

Frame 25 (110 bytes on wire, 110 bytes captured)
    Arrival Time: Apr 14, 2008 15:43:22.804236000
    [Time delta from previous captured frame: 0.628078000 seconds]
    [Time delta from previous displayed frame: 0.628078000 seconds]
    [Time since reference or first frame: 10.329861000 seconds]
    Frame Number: 25
    Frame Length: 110 bytes
    Capture Length: 110 bytes
    [Frame is marked: False]
    [Protocols in frame: eth:ip:udp:nbns]
    [Coloring Rule Name: SMB]
    [Coloring Rule String: smb || nbss || nbns || nbipx || ipxsap || netbios]
Ethernet II, Src: Dell_84:dc:61 (00:1c:23:84:dc:61), Dst: Broadcast (ff:ff:ff:ff:ff:ff)
Internet Protocol, Src: 10.10.10.58 (10.10.10.58), Dst: 10.255.255.255 (10.255.255.255)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
    Total Length: 96
    Identification: 0x0811 (2065)
    Flags: 0x00
    Fragment offset: 0
    Time to live: 128
    Protocol: UDP (0x11)
    Header checksum: 0x133a [correct]
    Source: 10.10.10.58 (10.10.10.58)
    Destination: 10.255.255.255 (10.255.255.255)
User Datagram Protocol, Src Port: netbios-ns (137), Dst Port: netbios-ns (137)
    Source port: netbios-ns (137)
    Destination port: netbios-ns (137)
    Length: 76
    Checksum: 0x543a [correct]
        [Good Checksum: True]
        [Bad Checksum: False]
NetBIOS Name Service
