LxNETES-3.2 patches
===================
Lx32patch4 (Lx32p4-eth_receive_data_fifo_overflow.sh) released 2006/08/04

implements ethernet errata for receive data fifo overflow bug
To apply the patch, just run "Lx32p4-eth_receive_data_fifo_overflow.sh" in an installed
LxNETES-32/ directory. Then recompile

"Lx32p4-eth_receive_data_fifo_overflow.sh" does not include precompiled binaries
For those take files from: images/

Tested with U-Boot 1.1.3 FS.2b

------------------------------------------------------------------------
known problems: booting from usb
