ID: 160
Name: del-5_7_2
Version: 2.00
Dependences: none
Description: Digi Embedded Linux 5.7.2 contains important fixes and updates.@@@@@@- Kernel@@@   - ccxmx51; Set IOMUX to be able to use SD2 for SD cards.@@@   - ccw9p9215, ccw9p2443; MAC assist fixes for piper memory corruption problem.@@@@@@- Root File System@@@   - save hwclock in UTC.@@@   - allow to mount EXT3/EXT4 filesystems.@@@   - update deprecated syntax in udev rule for JLink debugger.@@@@@@- Redpine wireless module (cwme9210, ccwmx51, ccwmx53)@@@   - update driver to version 3.2.10 (roaming fixes).@@@@@@- Piper wireless module (ccw9p9215)@@@   - fix wireless connection on band A@@@@@@- Documentation@@@   - Minor fixes
Minidescription: Digi Embedded Linux 5.7.2 upgrade
platformversion: 5.7
Revision: 1
platform: el
Relevance: RECOMMENDED
Filename: del-5_7_2_160.dipk
Date: 22/01/2013
Type: update
Target: environment
Size: 514kb
Installedsize: 2136kb
Checksum: f3ed0d78a2b9eb04784ec85812e72280
