ID: 145
Name: del-5_7_1
Version: 2.00
Dependences: none
Description: Digi Embedded Linux 5.7.1 contains important fixes and updates.@@@@@@Kernel@@@ * ccxmx51@@@    - Configure SD interfaces also for non wired platforms@@@    - mxc gpio. limit the set of gpio to one specific bit@@@    - adjust CS timing for SMSC911x Ethernet controller (impoves performance)@@@ * ccx9m2443@@@    - fix gpio assignation on serial port B@@@    - adjust CS timing for SMSC911x (impoves performance)@@@ * ccx9p9215, cxme9210@@@    - enable pull-ups of FIM SDIO interface@@@    - work aroung HW bug in 32 timer read function which might result in reads @@@      going backwards in time@@@@@@Root File System@@@  - set SUID for busybox on flash images@@@  - build flash images out of a temporary rootfs dir@@@  - make a cleaner reboot/halt@@@@@@Toolchain@@@  - gstreamer gst-fsl-plugin. fix image corruption on some gplay commands@@@@@@Documentation@@@  - remove High Speed I2C on MXC (not supported)
Minidescription: Digi Embedded Linux 5.7.1 upgrade
platformversion: 5.7
Revision: -1
platform: el
Relevance: RECOMMENDED
Filename: del-5_7_1_145.dipk
Date: 02/05/2012
Type: update
Target: environment
Size: 1130kb
Installedsize: 2679kb
Checksum: 00ec8b5eb46c762832d0a0280e93668d
