status message text
error message text
## XBee Configuration
Return to Network View
Extended Address: | 1 |
Product Type: | 1 |
Firmware Version: | 1 |
Unable to access the gateway RF module. Either there is no module installed or the installed module is not recognized. Settings are not configurable for this device.
### Basic Radio Settings
PAN ID (ID): |  | hex (0x0-0xffff, 0xffff=any PAN ID) |
Extended PAN ID (ID): |  | 8 hex bytes |
| Setting to 0 allows a random extended PAN ID to be used.
| Note: Changing the PAN ID may make this node inaccessible.
Node Identifier (NI): |  |  |
Discover Timeout (NT): |  | tenths of second (1-255) |
Scan Channels (SC): |  | hex (0xffff=all channels) |
Scan Duration (SD): |  | (0-7) |
### Advanced Radio Settings
Transmit Power Level (PL): |  |  |
Allows Join Time (NJ): |  | seconds (0-255. 255=always) |
CCA Threshold (CA): |  | -dBm (36-80) |
Random Delay Slots (RN): |  | (0-3, 0=disabled) |
Broadcast Hops (BH): |  | (0-30, 0=maximum) |
RSSI PWM (P0): |  | Enable RSSI PWM |
RSSI Timer (RP): |  | tenths of second (0-255) |
Associate LED (D5): |  |  |
| ### Serial Interface Settings
Baud Rate (BD): |  |  |
Parity (NB): |  |  |
Flow Control (D7): |  | Enable CTS Flow Control (DIO7) |
Packetization Timeout (RO): |  | msecs (0-255, 0=immediate) |
### Advanced Settings

Copyright © 1996-2006 Digi International, Inc. All rights reserved.