status message text
error message text
## XBee Configuration
### Network View of the XBee Devices ### Gateway Access ### Firmware Update Select a file containing firmware for the gateway radio module. Firmware files for ZNet 2.5 / ZB radios end with a .ebl extension. Firmware files for other radio types end with a .oem extension. Files ending with .zip or .ehx cannot be used on this page. The firmware version must be compatible with the gateway radio, and with other nodes on the network. If the gateway is enabled, most radio settings will be preserved during the firmware update. Some settings, such as encryption keys, may not be preserved and must be entered again. After the firmware is loaded successfully, the gateway radio will be restarted.
Radio Type: |  | 0x1901 (XBee)
Firmware: |  | 0x1141
Firmware File: |  |

Copyright © 1996-2006 Digi International, Inc. All rights reserved.

ZigBee not supported