Programmable XBee SDK

Release Notes (PN 93009415) 
Build 1.0.8
15 June, 2011

© 2011, Digi International
http://www.digi.com

Introduction
This document provides the latest Release information for the Programmable XBee SDK, which allows customers to easily develop applications for programmable XBee modules inside the CodeWarrior IDE.

Programmable XBee SDK v1.0.8, June 2011
Supported Hardware and Software
Hardware
The Programmable XBee SDK currently supports following Digi Programmable XBee modules:

•	XBee ZB (S2B) 
o	32KB flash memory
o	128KB flash memory
•	XBee ZB (S2C) 
o	32KB flash memory

Software
The Programmable XBee SDK currently supports following host Operating Systems:

•	Microsoft Windows XP/Vista/7
Changes with respect to previous version
•	First major release. Everything is new.
Known Issues and limitations
•	The Virtual EEPROM is not currently supported by the 128KB module variants.
•	Special considerations must be taken into account, regarding some special pins on the XBee ZB (S2B/S2C)

o	The RESET pin, when used as standard GPIO, has to be configured as input (due to a limitation of the 9S08QE).
o	The BKGD pin, when used as standard GPIO, has to be configured as output (due to a limitation of the 9S08QE).