Flash Update v2.02 - March 2000
Readme updated 9/21/01

This program requires that a Novell Server is present! 

This Program uses an IPX connection to download on Windows
95/98/NT/2000 systems. Install a new executable code version 
into your print server/network interface card (NIC). To 
run this program, both your workstation and the NIC must
have IPX (Novell) enabled.

On the network and you must have supervisor rights on
the Novell Server to use this program. Supervisory rights may
be added after installing Flash Update by right clicking on
the icon selecting properties. On the properties window select
The shortcut tab and you will see C:\NIC\FLASHUP\Flash_UP.EXE
Add to the string "NSSUPER". It should look exactly like the
Following example. ( C:\NIC\FLASHUP\FLASH_UP.EXE NSSUPER )


Once loaded, start this program, select the core image file 
to be downloaded, and then select the print server to which
the code is to be sent from the list of available units.
Units are listed by a three letter code, follows by the
six-digit serial number. 


This download program is used only for updating code
in the NIC's.
