This is version 1.50b of FTP Download.

This version has been updated on April 29, 2003

This release contains OTE309.BIN for updating 40.x, NET+ARM based
NIC designs that support our alternate MAC address feature.  It also
supports the Intel PHY.

This Program uses an FTP connection to download and 
install a new executable  code version into your print 
server/network interface card (NIC). To run this program, 
both your workstation and the NIC must have TCP/IP 
enabled and must have been assigned a  valid IP address.
If workstation and printer are on different subnets, 
subnet masks and default routers may also need to be 
entered.

Once loaded, start this program, select the core image file 
to be downloaded, and then enter the IP address of the 
print server to which the code is to be sent. The program 
will ask you for the maintenance password for this unit;
the default password is "sysadm". This password can be 
changed with standard NIC maintenance software.

This download program is used only for updating code
in the NIC's. It is suggested that, once NIC's have been 
downloaded, that this program be un-installed. Download 
programs will be shipped with any future code update.

The latest BIN files for use with the program are:

OTE104.BIN -> all 68340-based Ethernet NICs
OTE218.BIN -> All 12.0 and 12.1 NCC NICs (non-PCI)
OTE308.BIN -> All 15 40 and 50 NCC NICs
OTE309.BIN -> 40.x NICs supporting alternate MAC feature or Intel PHY
OTE400.BIN -> 12.1 PSIO with vector table in FLASH
OTE500.BIN -> All 12.1 and 40.x PCI based NICs
OTT100.BIN -> All old form-factor Token Ring NICs
OTT202.BIN -> All new form-factor Token Ring NICs

Other BIN files may be included for use with specific products
not listed here.

WARNING:
Do not attempt to print to the unit while updating the NIC.
Do not attempt to connect to the unit's HTML administrator
pages or telnet to the NIC while updating the NIC.
Do not power-cycle the unit while updating the NIC.
Failure to follow these instructions may cause the NIC firmware
to be improperly loaded. If this occurs, the NIC firmware must
be re-loaded at the factory.


