                     Release Notes 93000306_B1P   
                              for
                    Digi DataFire Sync2000 Adapters
                          Windows NT 4.0
                             v3.1.78
                       Release Date: 02/11/1999
		

Please reference the following number(s) when searching the Digi FTP/WWW
site for the latest software packages:
Software Image P/N 40001835_B1P

These numbers are for informational purposes only:
CD-ROM Software Image P/N 40001630_B1P

New Features:
1.	PPP protocol support
2.	Support for IBM Comm Server NT v6.01

Bug Fixes:
1.	SNA works in Half-Duplex mode.

2.	Diagnostic program SXBDiag is now being installed.

3.	System does not require reboots when SVC's are added.

4.	Installation performs cleanup when removing X.25 protocol. DigiWanX service
	is not left lying around.

5.	Various minor user interface bugs fixed.

Installation/User Interface:

1.	Currently simultaneously adding two or more adapters does not work. Adapters
	need to be added one board at a time.


2.	Within the wizard mode, if invalid input has been entered and back button is 
	pressed, an error message still appears indicating that the input is invalid.
	A valid input needs to be entered to be able to go back.



3.	The digi diver services  cannot be stopped from the control panel. This will
	be fixed in the final release of the driver. 

