### Installing the MS Loopback Adapter

This topic describes how to install the MS Loopback Adapter.

##### Procedure

1. From the Windows NT Control Panel, select Network.

   > The system displays the following prompt: Windows NT Networking is not installed. Do you want to install it now?

2. Click Yes.

   > The system asks if your computer is wired to the network or connected via Remote Access (modem).

3. Click Wired to the Network > Next > Select from list.

4. Select MS Loopback Adapter from the dialog box and then click Next.

5. Select NetBEUI as the network protocol and then click Next.

6. Choose to install the default network services by clicking Next > Next.

   > The system asks for a directory path.

7. Enter d:\i386\ (for Intel processors; use d:\alpha\ for Alpha systems) and load your Windows NT CD-ROM. (This assumes that your CD-ROM drive is drive D.)

   > The system asks you to specify a Frame Type.

8. Select 802.3 and then click Continue.

   > The network bindings page appears.

9. Click Next to accept the bindings and Next again to start the network.

10. Enter the name of your computer and workgroup and click Next.

11. Restart your computer to activate Windows NT Networking.

Copyright © 1999, Digi International. All rights reserved.