### Loading the NetWare Drivers for Xe Adapters

To load the driver automatically during boot, insert a load line in the AUTOEXEC.NCF file.

- Each Xe ISA adapter in the system must have its own load command.

- All load commands for ISA adapters must come before the PCI adapter load command.

Configure the driver by supplying values for these parameters after the load command:

| load aiodgxi port=xxx mem=xxxxx name=bname node=0

The parameters have these values:

port=xxx (required)

| Supply the adapter's unique 3 digit I/O port address as set by the dip switch on the adapter. Possible values: 100, 110, 120, 200, 220, 300, 320.

| Example: port=320

mem=xxxxx (required)

| Use this parameter to set the dual-port memory address for the adapter to use. You must choose a 32K block of free memory address space. Typically addresses from C0000 to D8000 are the best choice for availability.

| Possible values: 80000, 88000, 90000, 98000, A0000, A8000, B0000, B8000, C0000, C8000, D0000, D8000.

| Example: mem=d0000

name=bname (optional)

| Use this parameter to choose a name for the adapter. A name is assigned by the driver if you do not choose one.

| Possible values: Up to 10 alphanumerical characters.

| Example: name=digiboard1

node=0 (optional)

| Use this parameter, with this value, to tell the driver to number adapters sequentially, based on the order of the load lines in the AUTOEXEC.NCF file. This parameter must be used in the first load command. If not used, the adapters (and their ports) will be numbered based on the I/O address of the adapter (lowest to highest).

| Possible values: 0

| Example: node=0

Copyright © 1999, Digi International. All rights reserved.