### C/X ISA Host Adapter Specifications

Power Requirements
+5 volts +/- 5% | 2.0 amps typical
+12 volts +/- 5% | 40 milliamps typical
-12 volts +/- 5% | 40 milliamps typical
Environmental
Ambient temperature | 10 to 55 degrees C
Relative humidity | 5% to 90%
Air Movement | 30 CFM forced
Serial Interface Surge Suppression
Threshold voltage: | 13 volts (input signals)
5 volts (output signals)
Response time | < 10 nS
Mechanical
Length | 10.8 inches
Width | .6 inches
Height | 4.1 inches
Weight | 9 ounces

Copyright © 1999, Digi International. All rights reserved.