### SCO OpenServer Setup Overview

This Overview outlines the general procedure for installing and configuring the SCO OpenServer device driver for AccelePort asynchronous adapters.

1. Install the adapter. See the appropriate hardware installation card for more information.

2. Install the SCO UnixWare driver. See: Installing Driver Files for SCO OpenServer from CD or Installing Driver Files for SCO OpenServer from Diskette.
   The installation software creates devices in /dev. Click the applicable link to see the naming conventions for your adapter:

   - SCO OpenServer Port Names for C/X, EPC/X and Xem Systems

   - SCO OpenServer Port Names for Xr Adapters

   - SCO OpenServer Port Names for Xe Adapters

3. If you are using 8-pin RJ-45 connectors and need modem control signals, configure the ports for ALTPIN operation. See: Setting Up Ports for Use with 8-Pin RJ-45 Connectors.

4. AccelePort adapters support baud rates in excess of the maximum baud rate supported by Unix. To enable the use of these fast baud rates, a ditty parameter, fastbaud, has been provided. See: fastbaud Alternate Baud Rate Mapping.

5. If you have terminals with attached printers, the tty devices may be configured to support transparent printing. See About Transparent Printing for a general description of the process, and Transparent Printer Configuration for descriptions of the ditty parameters. For examples, click the applicable link:

   - Setup Examples for Transparent Printing - C/X, EPC/X, Xem

   - Setup Examples for Transparent Printing - Xr Adapters

   - Setup Examples for Transparent Printing - Xe Adapters

Copyright © 1999, Digi International. All rights reserved.