### Windows NT 4.0 Setup Overview

This Overview outlines the general procedure for installing and configuring the Windows NT device driver for AccelePort asynchronous adapters.

1. Install the adapter. See the appropriate hardware installation card for more information. If you are installing multiple PCI adapters, see: Installing Multiple PCI Adapters in Windows NT 4.0.

2. If Microsoft Networking has not been previously installed (for example, as part of a LAN card installation, or a previous AccelePort or DataFire installation), you must install the MS-Loopback adapter. See Installing the MS Loopback Adapter.

3. Install the Windows NT driver. See: Installing a Windows NT 4.0 Driver from CD, or Installing a Windows NT 4.0 Driver from Diskette.

4. Follow the prompts in the Configuration Wizard to set up the driver configuration.

Copyright © 1999, Digi International. All rights reserved.