### Windows 95/98 Setup Overview

This Overview outlines the general procedure for installing and configuring the Windows 95/98 device driver for AccelePort asynchronous adapters.

1. Install the Adapter. See the appropriate hardware installation card for more information.

2. Install the Device driver. See:

   - Installing PCI Drivers for Windows 95/98 from CD

   - Installing PCI Drivers for Windows 95/98 from Diskette

   - Installing ISA Drivers for Windows 95/98 from CD

   - Installing ISA Drivers for Windows 95/98 from Diskette

3. The Configuration Wizard assigns hardware resources automatically. If you are installing an ISA adapter, shut down the computer and set the adapter's DIP switches according to the resources assigned, or edit the assigned resources via the Control Panel-- See: Editing Assigned Hardware Resources in Windows 95/98.

4. If you wish to change the default port configurations, you can do this now. See: Editing Port Configurations in Windows 95/98. Note that in most cases this is unnecessary, since port configuration is usually handled by communications applications anyway.

Copyright © 1999, Digi International. All rights reserved.