### Installing PCI Drivers for Windows 95/98 from Diskette

#### Prerequisite

To install software on a computer that doesn't have a CD drive, you must create an installation diskette from the CD.

For instructions on creating installation diskettes, see:

Creating Installation and Diagnostic Diskettes

#### Procedure

1. Start Windows. Windows will detect the new hardware and prompt you to install software for it.

2. At the prompt to Select which driver you want to install..., select Driver from disk provided by hardware manufacturer and click OK. Specify the driver file location (A: for drive A) and click OK again.

3. Select the product you are installing from the displayed list.

4. The Ports Configuration properties page will now be displayed for you to view the assigned port names. For an Xem adapter, you will need to configure the PORTSTM modules that are connected to your adapter. On-line help is available for more information. When finished, click OK.

5. The Digi software is now installed. To activate it, restart your computer.

Copyright © 1999, Digi International. All rights reserved.