### EPC/X System Cables and Plugs

#### EIA-422 Cables

Twisted Pair Wire
Gage | 28 AWG, overall shield
Capacitance | 15.5 +/-3 pF/ft
Impedance | 100 ohms
Connectors
Male Connector | HD-15 subminiature
size 22 contacts
Female Connector | HD-15 subminature
size 22 contacts

#### EIA-422 Terminator

Connector: HD-15 subminiature male plug, size 22 contacts

| These pins are wired together:

| 1 - 6 2 -7 3 - 15 4 - 9 5 - 10 8 - 14

#### EIA-232 Loop Back Plugs

RJ45, 10 pin connector

| These pins are wired together:

| 3 - 1 - 8 5 - 6 9 - 2 - 10

DB-25, female connector

| These pins are wired together:

| 4 - 22 - 5 2 - 3 20 - 6 - 8

Copyright © 1999, Digi International. All rights reserved.