### Client-to-Server Modem Connections

Here are the steps required to set up a NetWare server to support client-to-server 56 Kbps modem connections.

#### Setup Overview

1. Install the driver. See one of the following: Installing NetWare Driver Files at the Server Console or Installing NetWare Driver Files from a Windows Client.

2. Configure RAS P/T/E using the dgrascfg utility. See Using Digi's dgrascfg Utility to Set Up a Line.

3. Configure client-to-server modem connections. See Configuring Client-to-Server Modems.

4. Configure applications to use 56 Kbps modems. See the application's documentation for information.

Copyright © 1999, Digi International. All rights reserved.