### SCO UnixWare Setup Overview

This Overview outlines the general procedure for installing and configuring the SCO UnixWare device driver for AccelePort asynchronous adapters.

1. Install the adapter. See the appropriate hardware installation card for more information.

2. Install the SCO UnixWare driver. See: Installing a SCO UnixWare Driver from CD or Installing a SCO UnixWare Driver from Diskettes.
   The installation software creates devices in /dev. Click the applicable link to see the naming conventions for your adapter:

   - SCO UnixWare Port Names for EPC/X, C/X, and Xem Systems

   - SCO UnixWare Port Names for Xr Adapters

   - SCO UnixWare Port Names for Xe Adapters

3. If you are using 8-pin RJ-45 connectors and need modem control signals, configure the ports for ALTPIN operation. See: Setting Up Ports for Use with 8-Pin RJ-45 Connectors.

4. AccelePort adapters support baud rates in excess of the maximum baud rate supported by Unix. To enable the use of these fast baud rates, a ditty parameter, fastbaud, has been provided. See: fastbaud Alternate Baud Rate Mapping.

5. If you have terminals with attached printers, the tty devices may be configured to support transparent printing. See About Transparent Printing for a general description of the process, and Transparent Printer Configuration for descriptions of the ditty parameters. For examples, click the applicable link:

   - Setup Examples for Transparent Printing - C/X, EPC/X, Xem

   - Setup Examples for Transparent Printing - Xr Adapters

   - Setup Examples for Transparent Printing - Xe Adapters

Copyright © 1999, Digi International. All rights reserved.