### Using Digi's dgrascfg Utility to Set Up a Line

This topic describes how to use the dgrascfg utility to set up your Digi RAS adapter for the line.

##### Procedure

1. At the command prompt, type the following: load dgrascfg.

2. Choose Configure/View Boards from the menu.

3. Highlight an adapter and press <Enter>.

4. Set up each port (line) on the adapter. Keep the following in mind:

   - Choose the parameters that match the provisioning of the line. For more information about parameters, press <F1> for online help.

   - Be sure to save the settings.

5. When configuration is complete exit dgrascfg and then down and restart the server.

Copyright © 1999, Digi International. All rights reserved.