### EPC/X PCI Host Adapter Specifications

Power Requirements
+5 volts +/- 5% | 1.8 amps typical
+12 volts +/- 5% | 20 milliamps typical
-12 volts +/- 5% | 20 milliamps typical
Environmental
Ambient temperature | 5 to 55 degrees C
Relative humidity | 20% to 80%
Air Movement | 30 CFM forced
Altitude | 0 to 12,000 feet
Serial Interface Surge Suppression
Threshold voltage: | 17 volts (input signals)
5 volts (output signals)
Response time | < 10 nS
Mechanical
Length | 6.785 inches
Width | .6 inches
Height | 4.5 inches
Weight | 12 ounces

Copyright © 1999, Digi International. All rights reserved.