### Installing a SCO UnixWare Driver from CD

Use this procedure to install a Digi SCO UnixWare driver from a CD.

#### Procedure

1. Place the CD in the system CD drive.

2. If it does not already exist, create a /usr/digi directory with this command:
   mkdir /usr/digi
   Note: The directory /usr/digi MUST be used.

3. Mount the CD drive using the following command:
   mount -r -f cdfs -o fperm=777 [devicename] /usr/digi
   where devicename is the name of the CD on your system. A common CD device name is: /dev/cd0

4. Change to the /usr/digi directory:
   cd /usr/digi

5. If you want to use the X Window System version of the Menu Program, ensure that X Window System is running.

6. Type one of the following at the command prompt:
   unix_xwin (X Windows version)
   unix_char (Curses version)

7. Choose the Install Software option (look under File in the curses version).

8. Select a driver from the list.
   The driver files are copied to the system.

9. Run Digi's MPI program to install the drivers. At the command prompt, enter:
   mpi
   The MPI program has useful help screens that describe in detail how to use the program and drivers. To access the help, press the <F1> key.

Copyright © 1999, Digi International. All rights reserved.