### SCO OpenServer Port Names for Xe Adapters

Format used for port names:

/dev/ttyi bp, /dev/pri bp

ttyi | Base name
pri | Base name for DigiPRINT ports
b | Adapter number (1-4)
p | Port Identifier (a-p, A-P) Lower case letters denote non modem control ports. These ports do not require DCD to be asserted before they can transmit data. Upper case letters denote modem control ports. These ports require DCD to be asserted before they can transmit data.

#### Example:

Port 4 of Adapter 2 is /dev/ttyi2d. The same port with modem control is /dev/ttyi2D. The corresponding DigiPRINT devices are /dev/pri2d and /dev/pri2D.

Copyright © 1999, Digi International. All rights reserved.