### AccelePort RAS 8 Specifications

Power Requirements
+5 volts +/- 5% | 1.5 amps typical
Environmental
Ambient Temperature | -10 to +60 degrees C
Relative Humidity | 5% to 90%
Air Movement | 30 CFM forced
Altitude | 0 to 12,000 feet (3657 m)
Mechanical
Length | 12.283 inches (31.2 cm)
Height | 4.2 inches (10.7 cm)
Weight | 9 ounces (252 g)

Copyright © 1999, Digi International. All rights reserved.