### Xem PCI Host Adapter Specifications

Power Requirements
+5 volts +/- 5% | .43 amps typical plus module power draw
Vio at +5 volts | 20 milliamps
Environmental
Ambient temperature | 10 to 55 degrees C
Relative humidity | 5% to 90%
Air Movement | 30 CFM forced
Altitude | 0 to 12,000 feet
Serial Interface Surge Suppression
Threshold voltage: | 13 volts
Response time | < 10 nS
Mechanical
Length | 6.75 inches
Width | .5 inches
Height | 4.2 inches
Weight | 4 ounces

Copyright © 1999, Digi International. All rights reserved.