### Configuring the ISDN CAPI Driver

This topic describes how to configure the Digi adapter to use an ISDN CAPI driver.

##### Procedure

1. Access the Internetworking Configuration menu. The following are paths to this menu:

   - For NIAS: Configure NIAS > Remote Access > Configure Synchronous Interfaces.

   - For MPR: Once inetcfg is loaded, the Internetworking Configuration menu appears.

   - For Connect: Configure Synchronous Interfaces.

2. Select Boards from the menu.

3. Configure a driver for each port on the Digi adapter. Do the following:

   - Choose WHSMCAPI from the Select a Driver list.

   - Choose DFCAPRAS from the Select a CAPI Driver list.

   - In the MAXPORTS field, specify the number of B-channels on the port.

   - In the Driver Specific Configuration field, associate the configuration with a line.

4. Down the server when ISDN CAPI driver configuration is completed.

Copyright © 1999, Digi International. All rights reserved.