### Digi RJ-45 Connector Pin Assignments

Signal | Description | DTE Use | Pin #
RI | Ring Indicator | Input | 1
DSR (DCD*) | Data Set Ready (Data Carrier Detect*) | Input | 2
RTS | Request to Send | Output | 3
GND | Chassis Ground | N/A | 4
TxD | Transmitted Data | Output | 5
RxD | Received Data | Input | 6
SG | Signal Ground | reference | 7
CTS | Clear to Send | Input | 8
DTR | Data Terminal Ready | Output | 9
DCD (DSR*) | Data Carrier Detect (Data Set Ready*) | Input | 10

| *When ALTPIN is in effect.

Copyright © 1999, Digi International. All rights reserved.